(footprint "alps_rkjxm1015004"
  (version 20240108) (generator "partreel")
  (layer "F.Cu")
  (descr "ALPS RKJXM1015004 8-directional stick switch with center push, single shaft, 11x11mm body, THT, automotive grade. Hole map per ALPS RKJXM catalog PC-board mounting hole drawing (p436-437), coordinates from the drawing vector geometry, cross-verified vs two independent field-built boards")
  (attr through_hole)
  (fp_text reference "SW" (at 0 -8.55) (layer "F.SilkS"))
  (fp_text value "RKJXM1015004" (at 0 8.55) (layer "F.Fab"))
  (pad "1" thru_hole circle (at 1.0 4.85) (size 1.8 1.8) (drill 1.1) (layers "*.Cu" "*.Mask"))
  (pad "2" thru_hole circle (at 4.85 -1.0) (size 1.8 1.8) (drill 1.1) (layers "*.Cu" "*.Mask"))
  (pad "3" thru_hole circle (at -1.0 -4.85) (size 1.8 1.8) (drill 1.1) (layers "*.Cu" "*.Mask"))
  (pad "4" thru_hole circle (at -4.85 1.0) (size 1.8 1.8) (drill 1.1) (layers "*.Cu" "*.Mask"))
  (pad "5" thru_hole circle (at 1.0 -5.255) (size 1.8 1.8) (drill 1.1) (layers "*.Cu" "*.Mask"))
  (pad "6" thru_hole circle (at 5.255 1.0) (size 1.8 1.8) (drill 1.1) (layers "*.Cu" "*.Mask"))
  (pad "7" thru_hole circle (at -5.255 -1.0) (size 1.8 1.8) (drill 1.1) (layers "*.Cu" "*.Mask"))
  (pad "8" thru_hole circle (at -1.0 5.255) (size 1.8 1.8) (drill 1.1) (layers "*.Cu" "*.Mask"))
  (pad "9" thru_hole circle (at -4.15 -2.7) (size 1.8 1.8) (drill 1.1) (layers "*.Cu" "*.Mask"))
  (pad "" np_thru_hole circle (at 1.0 -3.0) (size 1.2 1.2) (drill 1.2) (layers "F&B.Cu" "*.Mask"))
)
