(footprint "alps_rkjxt1f42001"
  (version 20240108) (generator "partreel")
  (layer "F.Cu")
  (descr "ALPS RKJXT1F42001 4-directional stick switch with encoder and center push, 17x17mm round body, THT. Hole map per ALPS RKJXT1F catalog Drawing No.1 (tolerance +/-0.1mm)")
  (attr through_hole)
  (fp_text reference "SW" (at 0 -10.6) (layer "F.SilkS"))
  (fp_text value "RKJXT1F42001" (at 0 10.6) (layer "F.Fab"))
  (pad "1" thru_hole circle (at -1.5 7.8) (size 1.8 1.8) (drill 1.1) (layers "*.Cu" "*.Mask"))
  (pad "2" thru_hole circle (at 7.8 1.5) (size 1.8 1.8) (drill 1.1) (layers "*.Cu" "*.Mask"))
  (pad "3" thru_hole circle (at 1.5 -7.8) (size 1.8 1.8) (drill 1.1) (layers "*.Cu" "*.Mask"))
  (pad "4" thru_hole circle (at -7.8 -1.5) (size 1.8 1.8) (drill 1.1) (layers "*.Cu" "*.Mask"))
  (pad "5" thru_hole circle (at -1.0 -5.78) (size 1.8 1.8) (drill 1.1) (layers "*.Cu" "*.Mask"))
  (pad "6" thru_hole circle (at 1.0 6.98) (size 1.8 1.8) (drill 1.1) (layers "*.Cu" "*.Mask"))
  (pad "7" thru_hole circle (at -7.8 1.5) (size 1.8 1.8) (drill 1.1) (layers "*.Cu" "*.Mask"))
  (pad "8" thru_hole circle (at 7.8 -1.5) (size 1.8 1.8) (drill 1.1) (layers "*.Cu" "*.Mask"))
  (pad "9" thru_hole circle (at -1.5 -7.8) (size 1.8 1.8) (drill 1.1) (layers "*.Cu" "*.Mask"))
  (pad "10" thru_hole circle (at 6.86 3.75) (size 1.8 1.8) (drill 1.1) (layers "*.Cu" "*.Mask"))
  (pad "" np_thru_hole circle (at -3.8 1.5) (size 1.2 1.2) (drill 1.2) (layers "F&B.Cu" "*.Mask"))
)
