(footprint "SW_435441019830_SMD"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -1.95 -2.85 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "SW_435441019830_SMD"
		(at -6.075 3.8 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -6.075 5.8 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -6.075 7 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -6.075 8.2 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.775 -2.05 90)
		(size 0.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "2" smd roundrect
		(at 0.825 -2.05 90)
		(size 0.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "3" smd roundrect
		(at 0.825 2.05 90)
		(size 0.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "4" smd roundrect
		(at -0.775 2.05 90)
		(size 0.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "SH" smd roundrect
		(at -1.4 0 90)
		(size 1.7 0.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(embedded_fonts no)
	(model "antmicro_435441019830.glb"
		(offset
			(xyz 0.025 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 -90)
		)
	)
)
