(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TPS7H5001-SP"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TPS7H5001-SP"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TPS7H5001-SP"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps7h5001-sp.pdf"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Radiation-hardened, QMLV and QMLP 2-MHz dual-output PWM controller with synchronous rectification"
				(at 35.56 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "5962R1822201PYE"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, SWITCHING, BUCK, VOLTAGE, REGULATOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "VQFN24_RGY_TEX VQFN24_RGY_TEX-M VQFN24_RGY_TEX-L"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TPS7H5001-SP_1_1"
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(name "RT")
					(number "1")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(name "PS")
					(number "2")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 2.54)
					(name "SP")
					(number "3")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 2.54)
					(name "LEB")
					(number "4")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(name "HICC")
					(number "5")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "SYNC")
					(number "6")
				)
				(pin passive line
					(at 22.86 -33.02 180)
					(length 2.54)
					(name "DCL")
					(number "7")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "EN")
					(number "8")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VIN")
					(number "9")
				)
				(pin passive line
					(at 22.86 0 180)
					(length 2.54)
					(name "OUTA")
					(number "10")
				)
				(pin passive line
					(at 22.86 -7.62 180)
					(length 2.54)
					(name "OUTB")
					(number "11")
				)
				(pin no_connect line
					(at 20.32 -36.83 180)
					(length 2.54)
					(name "NC")
					(number "12")
				)
				(pin no_connect line
					(at 20.32 -36.83 180)
					(length 2.54)
					(name "NC")
					(number "13")
				)
				(pin passive line
					(at 22.86 -10.16 180)
					(length 2.54)
					(name "SRB")
					(number "14")
				)
				(pin passive line
					(at 22.86 -2.54 180)
					(length 2.54)
					(name "SRA")
					(number "15")
				)
				(pin power_in line
					(at 0 -38.1 0)
					(length 2.54)
					(name "AVSS")
					(number "16")
				)
				(pin passive line
					(at 22.86 -27.94 180)
					(length 2.54)
					(name "VLDO")
					(number "17")
				)
				(pin passive line
					(at 22.86 -22.86 180)
					(length 2.54)
					(name "CS_ILIM")
					(number "18")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "FAULT")
					(number "19")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "REFCAP")
					(number "20")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 2.54)
					(name "RSC")
					(number "21")
				)
				(pin passive line
					(at 22.86 -17.78 180)
					(length 2.54)
					(name "SS")
					(number "22")
				)
				(pin passive line
					(at 22.86 -20.32 180)
					(length 2.54)
					(name "VSENSE")
					(number "23")
				)
				(pin passive line
					(at 22.86 -15.24 180)
					(length 2.54)
					(name "COMP")
					(number "24")
				)
			)
			(embedded_fonts no)
		)
)
