(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "74CBTLV3257_VQFN"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 34.29 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "74CBTLV3257_VQFN"
				(at 34.29 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "74CBTLV3257_VQFN"
				(at 34.29 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/916/74CBTLV3257-1318253.pdf"
				(at 34.29 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Interface analog switch/multiplexer/demultiplexer"
				(at 34.29 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "74CBTLV3257BQ,115"
				(at 34.29 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Nexperia"
				(at 34.29 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 34.29 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 34.29 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, LOGIC, IC, DECODER, ENCODER, MUX, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "74CBTLV3257_VQFN_1_1"
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "S")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "1B1")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "1B2")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "1A")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "2B1")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "2B2")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "2A")
					(number "7")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 2.54)
					(name "GND")
					(number "8")
				)
				(pin bidirectional line
					(at 20.32 0 180)
					(length 2.54)
					(name "3A")
					(number "9")
				)
				(pin bidirectional line
					(at 20.32 -2.54 180)
					(length 2.54)
					(name "3B2")
					(number "10")
				)
				(pin bidirectional line
					(at 20.32 -5.08 180)
					(length 2.54)
					(name "3B1")
					(number "11")
				)
				(pin bidirectional line
					(at 20.32 -7.62 180)
					(length 2.54)
					(name "4A")
					(number "12")
				)
				(pin bidirectional line
					(at 20.32 -10.16 180)
					(length 2.54)
					(name "4B2")
					(number "13")
				)
				(pin bidirectional line
					(at 20.32 -12.7 180)
					(length 2.54)
					(name "4B1")
					(number "14")
				)
				(pin input line
					(at 20.32 -15.24 180)
					(length 2.54)
					(name "OE")
					(number "15")
				)
				(pin power_in line
					(at 20.32 -17.78 180)
					(length 2.54)
					(name "VCC")
					(number "16")
				)
				(pin no_connect line
					(at 10.16 2.54 270)
					(length 2.54)
					(hide yes)
					(name "EP")
					(number "17")
				)
			)
			(embedded_fonts no)
		)
)
