(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "AP22615A_TSOT26"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 30.48 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "AP22615A_TSOT26"
				(at 30.48 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "AP22615A_TSOT26"
				(at 30.48 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/115/DIOD_S_A0008958405_1-2543193.pdf"
				(at 30.48 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Power Load Distribution Switch, High Side, Active High, 1 Output, 5.5 V, 3.6 A, 0.04 ohm, TSOT-26-6"
				(at 30.48 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "AP22615AWU-7"
				(at 30.48 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Diodes Incorporated"
				(at 30.48 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 30.48 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 30.48 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, VOLTAGE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "AP22615A_TSOT26_1_1"
				(pin power_out line
					(at 15.24 0 180)
					(length 2.54)
					(name "OUT")
					(number "1")
				)
				(pin power_in line
					(at 15.24 -5.08 180)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin output line
					(at 0 -2.54 0)
					(length 2.54)
					(name "FLG")
					(number "3")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "EN")
					(number "4")
				)
				(pin passive line
					(at 15.24 -2.54 180)
					(length 2.54)
					(name "ISET")
					(number "5")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "IN")
					(number "6")
				)
			)
			(embedded_fonts no)
		)
)
