(footprint "CTBGA-128_8x8mm_Layout14x14_P0.5x0.5mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -1 -4.65 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "CTBGA-128_8x8mm_Layout14x14_P0.5x0.5mm"
		(at -4.65 6.45 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -4.6 7.443 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -4.6 8.643 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -4.6 9.843 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -3.25 -3.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd circle
		(at -2.75 -3.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd circle
		(at -2.25 -3.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd circle
		(at -1.75 -3.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd circle
		(at -1.25 -3.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A6" smd circle
		(at -0.75 -3.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A7" smd circle
		(at -0.25 -3.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A8" smd circle
		(at 0.25 -3.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A9" smd circle
		(at 0.75 -3.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A10" smd circle
		(at 1.25 -3.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A11" smd circle
		(at 1.75 -3.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A12" smd circle
		(at 2.25 -3.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A13" smd circle
		(at 2.75 -3.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A14" smd circle
		(at 3.25 -3.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd circle
		(at -3.25 -2.74)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd circle
		(at -2.25 -2.74)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd circle
		(at -1.75 -2.74)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B5" smd circle
		(at -1.25 -2.74)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B6" smd circle
		(at -0.75 -2.74)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B7" smd circle
		(at -0.25 -2.74)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B8" smd circle
		(at 0.25 -2.74)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B9" smd circle
		(at 0.75 -2.74)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B10" smd circle
		(at 1.25 -2.74)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B11" smd circle
		(at 1.75 -2.74)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B12" smd circle
		(at 2.25 -2.74)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B14" smd circle
		(at 3.25 -2.74)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd circle
		(at -3.25 -2.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd circle
		(at -2.75 -2.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C13" smd circle
		(at 2.75 -2.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C14" smd circle
		(at 3.25 -2.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D1" smd circle
		(at -3.25 -1.74)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D2" smd circle
		(at -2.75 -1.74)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D5" smd circle
		(at -1.25 -1.74)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D6" smd circle
		(at -0.75 -1.74)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D7" smd circle
		(at -0.25 -1.74)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D8" smd circle
		(at 0.25 -1.74)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D9" smd circle
		(at 0.75 -1.74)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D10" smd circle
		(at 1.25 -1.74)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D13" smd circle
		(at 2.75 -1.74)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D14" smd circle
		(at 3.25 -1.74)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E1" smd circle
		(at -3.25 -1.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E2" smd circle
		(at -2.75 -1.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E4" smd circle
		(at -1.75 -1.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E11" smd circle
		(at 1.75 -1.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E13" smd circle
		(at 2.75 -1.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E14" smd circle
		(at 3.25 -1.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F1" smd circle
		(at -3.25 -0.74)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F2" smd circle
		(at -2.75 -0.74)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F4" smd circle
		(at -1.75 -0.74)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F7" smd circle
		(at -0.25 -0.74)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F8" smd circle
		(at 0.25 -0.74)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F11" smd circle
		(at 1.75 -0.74)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F13" smd circle
		(at 2.75 -0.74)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F14" smd circle
		(at 3.25 -0.74)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G1" smd circle
		(at -3.25 -0.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G2" smd circle
		(at -2.75 -0.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G4" smd circle
		(at -1.75 -0.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G6" smd circle
		(at -0.75 -0.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G9" smd circle
		(at 0.75 -0.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G11" smd circle
		(at 1.75 -0.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G13" smd circle
		(at 2.75 -0.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G14" smd circle
		(at 3.25 -0.24)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H1" smd circle
		(at -3.25 0.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H2" smd circle
		(at -2.75 0.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H4" smd circle
		(at -1.75 0.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H6" smd circle
		(at -0.75 0.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H9" smd circle
		(at 0.75 0.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H11" smd circle
		(at 1.75 0.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H13" smd circle
		(at 2.75 0.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H14" smd circle
		(at 3.25 0.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J1" smd circle
		(at -3.25 0.76)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J2" smd circle
		(at -2.75 0.76)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J4" smd circle
		(at -1.75 0.76)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J7" smd circle
		(at -0.25 0.76)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J8" smd circle
		(at 0.25 0.76)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J11" smd circle
		(at 1.75 0.76)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J13" smd circle
		(at 2.75 0.76)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J14" smd circle
		(at 3.25 0.76)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K1" smd circle
		(at -3.25 1.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K2" smd circle
		(at -2.75 1.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K4" smd circle
		(at -1.75 1.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K11" smd circle
		(at 1.75 1.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K13" smd circle
		(at 2.75 1.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K14" smd circle
		(at 3.25 1.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L1" smd circle
		(at -3.25 1.76)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L2" smd circle
		(at -2.75 1.76)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L5" smd circle
		(at -1.25 1.76)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L6" smd circle
		(at -0.75 1.76)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L7" smd circle
		(at -0.25 1.76)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L8" smd circle
		(at 0.25 1.76)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L9" smd circle
		(at 0.75 1.76)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L10" smd circle
		(at 1.25 1.76)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L13" smd circle
		(at 2.75 1.76)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L14" smd circle
		(at 3.25 1.76)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M1" smd circle
		(at -3.25 2.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M2" smd circle
		(at -2.75 2.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M13" smd circle
		(at 2.75 2.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M14" smd circle
		(at 3.25 2.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N1" smd circle
		(at -3.25 2.76)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N3" smd circle
		(at -2.25 2.76)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N4" smd circle
		(at -1.75 2.76)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N5" smd circle
		(at -1.25 2.76)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N6" smd circle
		(at -0.75 2.76)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N7" smd circle
		(at -0.25 2.76)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N8" smd circle
		(at 0.25 2.76)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N9" smd circle
		(at 0.75 2.76)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N10" smd circle
		(at 1.25 2.76)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N11" smd circle
		(at 1.75 2.76)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N12" smd circle
		(at 2.25 2.76)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N14" smd circle
		(at 3.25 2.76)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P1" smd circle
		(at -3.25 3.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P2" smd circle
		(at -2.75 3.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P3" smd circle
		(at -2.25 3.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P4" smd circle
		(at -1.75 3.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P5" smd circle
		(at -1.25 3.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P6" smd circle
		(at -0.75 3.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P7" smd circle
		(at -0.25 3.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P8" smd circle
		(at 0.25 3.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P9" smd circle
		(at 0.75 3.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P10" smd circle
		(at 1.25 3.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P11" smd circle
		(at 1.75 3.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P12" smd circle
		(at 2.25 3.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P13" smd circle
		(at 2.75 3.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P14" smd circle
		(at 3.25 3.26)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_as3722.glb"
		(offset
			(xyz 0 0 -0.2)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
