(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "AS3722"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 55.88 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "AS3722"
				(at 55.88 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "AS3722"
				(at 55.88 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://look.ams-osram.com/m/21ab19a43cbbe57a/original/AS3722-DS000358.pdf"
				(at 55.88 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Programmable power management unit, 4x DC-DC buck converter, 3x buck converter (6A to 24A), 11 low noise LDOs, 4MHz switching frequency, RTC"
				(at 55.88 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "AMS"
				(at 55.88 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "AS3722"
				(at 55.88 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 55.88 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 55.88 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "IC,DC-DC,LDO,ADC,I2C,SPI"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "AS3722_1_1"
				(pin power_in line
					(at 38.1 -45.72 180)
					(length 3.81)
					(name "VSSA")
					(number "A1")
				)
				(pin passive line
					(at 38.1 -45.72 180)
					(length 3.81)
					(name "VSSA")
					(number "A14")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 3.81)
					(name "ONKEY")
					(number "B10")
				)
				(pin output line
					(at 38.1 -7.62 180)
					(length 3.81)
					(name "XINT")
					(number "C1")
				)
				(pin output clock
					(at 38.1 -17.78 180)
					(length 3.81)
					(name "CLK32K")
					(number "D1")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 3.81)
					(name "LID")
					(number "D7")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 3.81)
					(name "THERM")
					(number "D8")
				)
				(pin output line
					(at 38.1 -10.16 180)
					(length 3.81)
					(name "OC_PG")
					(number "E1")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 3.81)
					(name "ENABLE2")
					(number "E11")
				)
				(pin passive line
					(at 38.1 -45.72 180)
					(length 3.81)
					(name "VSSA")
					(number "F7")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 3.81)
					(name "ENABLE1")
					(number "F8")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 3.81)
					(name "XIN32K")
					(number "G1")
				)
				(pin output line
					(at 0 -38.1 0)
					(length 3.81)
					(name "XOUT32K")
					(number "G2")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VSUP_ANA")
					(number "H1")
				)
				(pin output line
					(at 38.1 0 180)
					(length 3.81)
					(name "V2_5")
					(number "H2")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VBAT_BKUP")
					(number "H4")
				)
				(pin bidirectional line
					(at 38.1 -33.02 180)
					(length 3.81)
					(name "RBIAS")
					(number "J2")
				)
				(pin bidirectional line
					(at 38.1 -27.94 180)
					(length 3.81)
					(name "CREF")
					(number "J4")
				)
				(pin passive line
					(at 38.1 -45.72 180)
					(length 3.81)
					(name "VSSA")
					(number "J7")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 3.81)
					(name "XRES_IN")
					(number "J8")
				)
				(pin power_in line
					(at 38.1 -43.18 180)
					(length 3.81)
					(name "GNDSENSE")
					(number "K4")
				)
				(pin output line
					(at 0 -30.48 0)
					(length 3.81)
					(name "XRES_OUT")
					(number "L5")
				)
				(pin output line
					(at 38.1 -5.08 180)
					(length 3.81)
					(name "EN5V")
					(number "L6")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "VBAT")
					(number "L7")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 3.81)
					(name "AC_OK")
					(number "L8")
				)
				(pin passive line
					(at 38.1 -45.72 180)
					(length 3.81)
					(name "VSSA")
					(number "P1")
				)
				(pin passive line
					(at 38.1 -45.72 180)
					(length 3.81)
					(name "VSSA")
					(number "P14")
				)
			)
			(symbol "AS3722_2_1"
				(pin bidirectional line
					(at 40.64 -10.16 180)
					(length 3.81)
					(name "GPIO4")
					(number "B3")
				)
				(pin bidirectional line
					(at 40.64 -15.24 180)
					(length 3.81)
					(name "GPIO6")
					(number "B4")
				)
				(pin input clock
					(at 0 -15.24 0)
					(length 3.81)
					(name "PWM_CLK2_ADC1")
					(number "B11")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 3.81)
					(name "PWM_DAT2_ADC2")
					(number "B12")
				)
				(pin bidirectional line
					(at 40.64 -12.7 180)
					(length 3.81)
					(name "GPIO5")
					(number "C2")
				)
				(pin bidirectional line
					(at 40.64 -17.78 180)
					(length 3.81)
					(name "GPIO7")
					(number "D2")
				)
				(pin bidirectional line
					(at 40.64 -5.08 180)
					(length 3.81)
					(name "GPIO2")
					(number "D5")
				)
				(pin bidirectional line
					(at 40.64 0 180)
					(length 3.81)
					(name "GPIO0")
					(number "D6")
				)
				(pin input clock
					(at 0 -12.7 0)
					(length 3.81)
					(name "PWM_CLK1")
					(number "D9")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 3.81)
					(name "PWM_DAT1")
					(number "D10")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "ENABLE3_SDO")
					(number "E2")
				)
				(pin bidirectional line
					(at 40.64 -7.62 180)
					(length 3.81)
					(name "GPIO3")
					(number "E4")
				)
				(pin power_in line
					(at 40.64 -27.94 180)
					(length 3.81)
					(name "VSS_GPIO")
					(number "F1")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "VDD_GPIO_LV")
					(number "F2")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 3.81)
					(name "SDA_SDI")
					(number "F4")
				)
				(pin input clock
					(at 0 -22.86 0)
					(length 3.81)
					(name "SCL_SCLK")
					(number "G4")
				)
				(pin bidirectional line
					(at 40.64 -2.54 180)
					(length 3.81)
					(name "GPIO1")
					(number "G6")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 3.81)
					(name "SCSB")
					(number "H6")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VSUP_GPIO")
					(number "L9")
				)
			)
			(symbol "AS3722_3_1"
				(pin power_out line
					(at 27.94 -10.16 180)
					(length 3.81)
					(name "LDO4")
					(number "A2")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 3.81)
					(name "VIN_LDO3_4")
					(number "A3")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 3.81)
					(name "VIN_LDO3_SW")
					(number "A4")
				)
				(pin power_out line
					(at 27.94 -20.32 180)
					(length 3.81)
					(name "LDO9")
					(number "A5")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VIN_LDO9_10")
					(number "A6")
				)
				(pin power_out line
					(at 27.94 -15.24 180)
					(length 3.81)
					(name "LDO6")
					(number "A7")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "VIN_LDO1_6")
					(number "A8")
				)
				(pin power_out line
					(at 27.94 -5.08 180)
					(length 3.81)
					(name "LDO2")
					(number "A9")
				)
				(pin power_out line
					(at 27.94 -12.7 180)
					(length 3.81)
					(name "LDO5")
					(number "A10")
				)
				(pin power_out line
					(at 27.94 -17.78 180)
					(length 3.81)
					(name "LDO7")
					(number "A11")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 3.81)
					(name "VIN_LDO2_5_7")
					(number "A12")
				)
				(pin power_out line
					(at 27.94 0 180)
					(length 3.81)
					(name "LDO0")
					(number "A13")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 3.81)
					(name "VIN_LDO11")
					(number "B1")
				)
				(pin power_out line
					(at 27.94 -25.4 180)
					(length 3.81)
					(name "LDO11")
					(number "B5")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 3.81)
					(name "VIN_LDO3_LV")
					(number "B6")
				)
				(pin power_out line
					(at 27.94 -7.62 180)
					(length 3.81)
					(name "LDO3")
					(number "B7")
				)
				(pin power_out line
					(at 27.94 -22.86 180)
					(length 3.81)
					(name "LDO10")
					(number "B8")
				)
				(pin power_out line
					(at 27.94 -2.54 180)
					(length 3.81)
					(name "LDO1")
					(number "B9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VIN_LDO0")
					(number "B14")
				)
			)
			(symbol "AS3722_4_1"
				(text "DCDC0"
					(at 16.51 -20.32 900)
				)
				(text "DCDC1"
					(at 16.51 -45.72 900)
				)
				(text "DCDC2"
					(at 16.51 -58.42 900)
				)
				(text "DCDC3"
					(at 26.67 -6.35 900)
				)
				(text "DCDC4"
					(at 26.67 -20.32 900)
				)
				(text "DCDC5"
					(at 26.67 -38.1 900)
				)
				(text "DCDC6"
					(at 26.67 -58.42 900)
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 3.81)
					(name "CTRL1_SD6")
					(number "C13")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 3.81)
					(name "CTRL2_SD6")
					(number "C14")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 3.81)
					(name "CTRL1_SD1")
					(number "D13")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 3.81)
					(name "CTRL2_SD1")
					(number "D14")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "CTRL1_SD0")
					(number "E13")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "CTRL2_SD0")
					(number "E14")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 3.81)
					(name "FB_SD6_P")
					(number "F11")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "CTRL3_SD0")
					(number "F13")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "CTRL4_SD0")
					(number "F14")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 3.81)
					(name "FB_SD1_P")
					(number "G9")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 3.81)
					(name "FB_SD6_N")
					(number "G11")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "CTRL5_SD0")
					(number "G13")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "CTRL6_SD0")
					(number "G14")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 3.81)
					(name "FB_SD1_N")
					(number "H9")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "FB_SDO_P")
					(number "H11")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "CTRL7_SD0")
					(number "H13")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "CTRL8_SD0")
					(number "H14")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 3.81)
					(name "FB_SD5")
					(number "J1")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "FB_SDO_N")
					(number "J11")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "TEMP2_SD0")
					(number "J13")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "TEMP1_SD0")
					(number "J14")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 3.81)
					(name "FB_SD2")
					(number "K1")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 3.81)
					(name "FB_SD3")
					(number "K2")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "TEMP4_SD0")
					(number "K11")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "TEMP3_SD0")
					(number "K13")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "TEMP_SD1")
					(number "K14")
				)
				(pin power_in line
					(at 43.18 0 180)
					(length 3.81)
					(name "VSUP_SD3")
					(number "L1")
				)
				(pin passive line
					(at 43.18 0 180)
					(length 3.81)
					(name "VSUP_SD3")
					(number "L2")
				)
				(pin bidirectional line
					(at 43.18 -19.05 180)
					(length 3.81)
					(name "FB_SD4")
					(number "L10")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 3.81)
					(name "TEMP2_SD6")
					(number "L13")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 3.81)
					(name "TEMP1_SD6")
					(number "L14")
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 3.81)
					(name "LX_SD3")
					(number "M1")
				)
				(pin passive line
					(at 43.18 -2.54 180)
					(length 3.81)
					(name "LX_SD3")
					(number "M2")
				)
				(pin power_in line
					(at 43.18 -21.59 180)
					(length 3.81)
					(name "VSS_SD4")
					(number "M13")
				)
				(pin passive line
					(at 43.18 -21.59 180)
					(length 3.81)
					(name "VSS_SD4")
					(number "M14")
				)
				(pin passive line
					(at 43.18 -2.54 180)
					(length 3.81)
					(name "LX_SD3")
					(number "N1")
				)
				(pin power_in line
					(at 43.18 -7.62 180)
					(length 3.81)
					(name "VSS_SD3")
					(number "N3")
				)
				(pin power_in line
					(at 0 -60.96 0)
					(length 3.81)
					(name "VSS_SD2")
					(number "N4")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 3.81)
					(name "LX_SD2")
					(number "N5")
				)
				(pin power_in line
					(at 0 -53.34 0)
					(length 3.81)
					(name "VSUP_SD2")
					(number "N6")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(name "LX_SD2")
					(number "N7")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 3.81)
					(name "VSS_SD2")
					(number "N8")
				)
				(pin power_in line
					(at 43.18 -38.1 180)
					(length 3.81)
					(name "VSS_SD5")
					(number "N9")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 3.81)
					(name "LX_SD5")
					(number "N10")
				)
				(pin power_in line
					(at 43.18 -30.48 180)
					(length 3.81)
					(name "VSUP_SD5")
					(number "N11")
				)
				(pin power_in line
					(at 43.18 -13.97 180)
					(length 3.81)
					(name "VSUP_SD4")
					(number "N12")
				)
				(pin bidirectional line
					(at 43.18 -16.51 180)
					(length 3.81)
					(name "LX_SD4")
					(number "N14")
				)
				(pin passive line
					(at 43.18 -7.62 180)
					(length 3.81)
					(name "VSS_SD3")
					(number "P2")
				)
				(pin passive line
					(at 43.18 -7.62 180)
					(length 3.81)
					(name "VSS_SD3")
					(number "P3")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 3.81)
					(name "VSS_SD2")
					(number "P4")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(name "LX_SD2")
					(number "P5")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(name "VSUP_SD2")
					(number "P6")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(name "LX_SD2")
					(number "P7")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 3.81)
					(name "VSS_SD2")
					(number "P8")
				)
				(pin passive line
					(at 43.18 -38.1 180)
					(length 3.81)
					(name "VSS_SD5")
					(number "P9")
				)
				(pin passive line
					(at 43.18 -33.02 180)
					(length 3.81)
					(name "LX_SD5")
					(number "P10")
				)
				(pin passive line
					(at 43.18 -30.48 180)
					(length 3.81)
					(name "VSUP_SD5")
					(number "P11")
				)
				(pin passive line
					(at 43.18 -13.97 180)
					(length 3.81)
					(name "VSUP_SD4")
					(number "P12")
				)
				(pin passive line
					(at 43.18 -16.51 180)
					(length 3.81)
					(name "LX_SD4")
					(number "P13")
				)
			)
			(embedded_fonts no)
		)
)
