(footprint "SW_DIP_SPSTx02_Slide_Copal_CVS-02xB_W5.9mm_P1mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "SMD 2x-dip-switch SPST Copal_CVS-02xB, Slide, row spacing 5.9 mm")
	(tags "SMD DIP Switch SPST Slide 5.9mm")
	(property "Reference" "REF**"
		(at 0 -2.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_DIP_SPSTx02_Slide_Copal_CVS-02xB_W5.9mm_P1mm"
		(at 0 2.91 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -3.6 4.91 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -3.6 5.908 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -3.6 6.908 0)
		(layer "F.Fab")
	)
	(fp_text user "on"
		(at 2.05 0.72 270)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -2.95 -0.5)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.95 0.5)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 2.95 0.5)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 2.95 -0.5)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -2.15 -1.5)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -2.15 1.5)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 2.15 -1.5)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 2.15 1.5)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_cvs_02b.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 90)
		)
	)
)
