(footprint "SW_DIP_SPSTx08_Slide_Copal_CVS-08xB_W5.9mm_P1mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "SMD 8x-dip-switch SPST Copal_CVS-08xB, Slide, row spacing 5.9 mm (232 mils), body size  (see http://www.nidec-copal-electronics.com/e/catalog/switch/cvs.pdf)")
	(tags "SMD DIP Switch SPST Slide 5.9mm 232mil")
	(property "Reference" "REF**"
		(at -3.71 -5.11 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_DIP_SPSTx08_Slide_Copal_CVS-08xB_W5.9mm_P1mm"
		(at -14.59 6.29 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -14.59 8.29 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -14.59 10.69 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -14.59 11.89 0)
		(layer "F.Fab")
	)
	(fp_text user "on"
		(at 1.98 0.71 270)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -2.952 -3.5)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.952 -2.5)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -2.952 -1.5)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -2.952 -0.5)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -2.952 0.498)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -2.952 1.499)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -2.952 2.499)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -2.952 3.499)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 2.95 3.499)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 2.95 2.499)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 2.95 1.499)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 2.95 0.498)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 2.95 -0.5)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 2.95 -1.5)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 2.95 -2.5)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 2.95 -3.5)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -2.15 -4.5)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -2.15 4.498)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 2.148 -4.5)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 2.148 4.498)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_cvs_08tb.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 90)
		)
	)
)
