(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SW_CVS-08TB"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "SW"
				(at 26.67 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SW_CVS-08TB"
				(at 26.67 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Footprint" "SW_CVS-08TB"
				(at 26.67 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/972/cvs-1827291.pdf"
				(at 26.67 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "DIP / SIP Switch, 8 Circuits, Slide, Surface Mount, SPST, 6 V, 100 mA"
				(at 26.67 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "CVS-08TB"
				(at 26.67 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Nidec Components"
				(at 26.67 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 26.67 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 26.67 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SWITCH, SLIDE, SPST, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "SW?DIP?x2*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SW_CVS-08TB_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "")
					(number "2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "")
					(number "3")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "")
					(number "4")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "")
					(number "5")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "")
					(number "6")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "")
					(number "7")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(name "")
					(number "8")
				)
				(pin passive line
					(at 12.7 -17.78 180)
					(length 2.54)
					(name "")
					(number "9")
				)
				(pin passive line
					(at 12.7 -15.24 180)
					(length 2.54)
					(name "")
					(number "10")
				)
				(pin passive line
					(at 12.7 -12.7 180)
					(length 2.54)
					(name "")
					(number "11")
				)
				(pin passive line
					(at 12.7 -10.16 180)
					(length 2.54)
					(name "")
					(number "12")
				)
				(pin passive line
					(at 12.7 -7.62 180)
					(length 2.54)
					(name "")
					(number "13")
				)
				(pin passive line
					(at 12.7 -5.08 180)
					(length 2.54)
					(name "")
					(number "14")
				)
				(pin passive line
					(at 12.7 -2.54 180)
					(length 2.54)
					(name "")
					(number "15")
				)
				(pin passive line
					(at 12.7 0 180)
					(length 2.54)
					(name "")
					(number "16")
				)
				(pin power_in line
					(at 12.7 -20.32 180)
					(length 2.54)
					(name "SH")
					(number "17")
				)
			)
			(embedded_fonts no)
		)
)
