(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "FSUSB30MUX"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "FSUSB30MUX"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "FSUSB30MUX"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/fsusb30-d.pdf"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Special purpose interface switch"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "FSUSB30MUX"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "ON Semiconductor"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "FSUSB30MUX_1_1"
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "S")
					(number "1")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 2.54)
					(name "D1+")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "D2+")
					(number "3")
				)
				(pin bidirectional line
					(at 21.59 -2.54 180)
					(length 2.54)
					(name "D+")
					(number "4")
				)
				(pin power_in line
					(at 21.59 -20.32 180)
					(length 2.54)
					(name "GND")
					(number "5")
				)
				(pin bidirectional line
					(at 21.59 -11.43 180)
					(length 2.54)
					(name "D-")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 2.54)
					(name "D2-")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 2.54)
					(name "D1-")
					(number "8")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "~{OE}")
					(number "9")
				)
				(pin power_in line
					(at 21.59 1.27 180)
					(length 2.54)
					(name "VCC")
					(number "10")
				)
			)
			(embedded_fonts no)
		)
)
