(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "KSZ9567STXI"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 55.88 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "KSZ9567STXI"
				(at 55.88 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "KSZ9567STXI"
				(at 55.88 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.arrow.com/en/products/ksz9567stxi/microchip-technology"
				(at 55.88 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Ethernet ICs 7-Port Gigabit Ethernet Switch with SGMII, IEEE 1588 v2, AVB, EEE, WOL, QoS, LinkMD, Industrial temp."
				(at 55.88 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "KSZ9567STXI"
				(at 55.88 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 55.88 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 55.88 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 55.88 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT, TRANSCEIVER, IC, ETHERNET, PHY, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "KSZ9567STXI_1_1"
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(hide yes)
					(name "AVDDL")
					(number "3")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "AVDDH")
					(number "10")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "DVDDL")
					(number "11")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(hide yes)
					(name "AVDDL")
					(number "14")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(hide yes)
					(name "AVDDL")
					(number "19")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "AVDDH")
					(number "22")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "DVDDL")
					(number "23")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(hide yes)
					(name "AVDDL")
					(number "30")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "AVDDH")
					(number "33")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(hide yes)
					(name "AVDDL")
					(number "36")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(hide yes)
					(name "AVDDL")
					(number "41")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "AVDDH")
					(number "44")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "DVDDL")
					(number "45")
				)
				(pin passive line
					(at 30.48 -52.07 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "46")
				)
				(pin passive line
					(at 30.48 -52.07 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "47")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "DVDDL")
					(number "56")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 3.81)
					(hide yes)
					(name "VDDIO")
					(number "61")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "DVDDL")
					(number "66")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 3.81)
					(name "IBA")
					(number "67")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 3.81)
					(hide yes)
					(name "VDDIO")
					(number "68")
				)
				(pin passive line
					(at 30.48 -52.07 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "69")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "DVDDL")
					(number "70")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "VDDLS")
					(number "71")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDDHS")
					(number "72")
				)
				(pin no_connect line
					(at 26.67 -46.99 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "73")
				)
				(pin no_connect line
					(at 26.67 -46.99 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "74")
				)
				(pin passive line
					(at 30.48 -52.07 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "75")
				)
				(pin passive line
					(at 30.48 -52.07 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "77")
				)
				(pin passive line
					(at 30.48 -52.07 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "80")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "VDDHS")
					(number "83")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 3.81)
					(name "VDDLS")
					(number "84")
				)
				(pin bidirectional line
					(at 30.48 -17.78 180)
					(length 3.81)
					(name "LED4_0")
					(number "85")
				)
				(pin bidirectional line
					(at 30.48 -20.32 180)
					(length 3.81)
					(name "LED4_1")
					(number "86")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "DVDDL")
					(number "87")
				)
				(pin bidirectional line
					(at 30.48 -12.7 180)
					(length 3.81)
					(name "LED3_0")
					(number "88")
				)
				(pin bidirectional line
					(at 30.48 -15.24 180)
					(length 3.81)
					(name "LED3_1")
					(number "89")
				)
				(pin bidirectional line
					(at 30.48 0 180)
					(length 3.81)
					(name "GPIO_1")
					(number "90")
				)
				(pin bidirectional line
					(at 30.48 -7.62 180)
					(length 3.81)
					(name "LED2_0")
					(number "91")
				)
				(pin bidirectional line
					(at 30.48 -10.16 180)
					(length 3.81)
					(name "LED2_1")
					(number "92")
				)
				(pin output line
					(at 0 -24.13 0)
					(length 3.81)
					(name "~{PME}")
					(number "93")
				)
				(pin output line
					(at 0 -21.59 0)
					(length 3.81)
					(name "~{INTRP}")
					(number "94")
				)
				(pin output line
					(at 0 -45.72 0)
					(length 3.81)
					(name "SYNCLKO")
					(number "95")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 3.81)
					(name "~{RESET}")
					(number "96")
				)
				(pin output line
					(at 0 -41.91 0)
					(length 3.81)
					(name "SDO")
					(number "97")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 3.81)
					(name "SDI")
					(number "98")
					(alternate "MDIO" passive line)
					(alternate "SDA" passive line)
				)
				(pin power_in line
					(at 0 -6.35 0)
					(length 3.81)
					(name "VDDIO")
					(number "99")
				)
				(pin input line
					(at 0 -34.29 0)
					(length 3.81)
					(name "~{SCS}")
					(number "100")
				)
				(pin input line
					(at 0 -36.83 0)
					(length 3.81)
					(name "SCL")
					(number "101")
					(alternate "MDC" passive line)
				)
				(pin bidirectional line
					(at 30.48 -22.86 180)
					(length 3.81)
					(name "LED5_0")
					(number "102")
				)
				(pin bidirectional line
					(at 30.48 -25.4 180)
					(length 3.81)
					(name "LED5_1")
					(number "103")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 3.81)
					(name "DVDDL")
					(number "104")
				)
				(pin bidirectional line
					(at 30.48 -2.54 180)
					(length 3.81)
					(name "LED1_0")
					(number "105")
				)
				(pin bidirectional line
					(at 30.48 -5.08 180)
					(length 3.81)
					(name "LED1_1")
					(number "106")
				)
				(pin power_in line
					(at 30.48 -52.07 180)
					(length 3.81)
					(name "GND")
					(number "107")
				)
				(pin no_connect line
					(at 26.67 -46.99 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "108")
				)
				(pin passive line
					(at 30.48 -52.07 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "109")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "DVDDL")
					(number "110")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "AVDDH")
					(number "111")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 3.81)
					(name "AVDDL")
					(number "114")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(hide yes)
					(name "AVDDL")
					(number "119")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "AVDDH")
					(number "122")
				)
				(pin passive line
					(at 30.48 -52.07 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "123")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(hide yes)
					(name "AVDDL")
					(number "124")
				)
				(pin output line
					(at 0 -52.07 0)
					(length 3.81)
					(name "XO")
					(number "125")
				)
				(pin input line
					(at 0 -49.53 0)
					(length 3.81)
					(name "XI")
					(number "126")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 3.81)
					(name "ISET")
					(number "127")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "AVDDH")
					(number "128")
				)
				(pin power_in line
					(at 30.48 -49.53 180)
					(length 3.81)
					(name "EP")
					(number "129")
				)
			)
			(symbol "KSZ9567STXI_2_1"
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "TXRX1_A_P")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "TXRX1_A_N")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "TXRX1_B_P")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "TXRX1_B_N")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "TXRX1_C_P")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "TXRX1_C_N")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "TXRX1_D_P")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "TXRX1_D_N")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 3.81)
					(name "TXRX2_A_P")
					(number "12")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 3.81)
					(name "TXRX2_A_N")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 3.81)
					(name "TXRX2_B_P")
					(number "15")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 3.81)
					(name "TXRX2_B_N")
					(number "16")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 3.81)
					(name "TXRX2_C_P")
					(number "17")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 3.81)
					(name "TXRX2_C_N")
					(number "18")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 3.81)
					(name "TXRX2_D_P")
					(number "20")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 3.81)
					(name "TXRX2_D_N")
					(number "21")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 3.81)
					(name "TXRX3_A_P")
					(number "24")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 3.81)
					(name "TXRX3_A_N")
					(number "25")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 3.81)
					(name "TXRX3_B_P")
					(number "26")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 3.81)
					(name "TXRX3_B_N")
					(number "27")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 3.81)
					(name "TXRX3_C_P")
					(number "28")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 3.81)
					(name "TXRX3_C_N")
					(number "29")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 3.81)
					(name "TXRX3_D_P")
					(number "31")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 3.81)
					(name "TXRX3_D_N")
					(number "32")
				)
				(pin bidirectional line
					(at 0 -82.55 0)
					(length 3.81)
					(name "TXRX4_A_P")
					(number "34")
				)
				(pin bidirectional line
					(at 0 -80.01 0)
					(length 3.81)
					(name "TXRX4_A_N")
					(number "35")
				)
				(pin bidirectional line
					(at 0 -77.47 0)
					(length 3.81)
					(name "TXRX4_B_P")
					(number "37")
				)
				(pin bidirectional line
					(at 0 -74.93 0)
					(length 3.81)
					(name "TXRX4_B_N")
					(number "38")
				)
				(pin bidirectional line
					(at 0 -72.39 0)
					(length 3.81)
					(name "TXRX4_C_P")
					(number "39")
				)
				(pin bidirectional line
					(at 0 -69.85 0)
					(length 3.81)
					(name "TXRX4_C_N")
					(number "40")
				)
				(pin bidirectional line
					(at 0 -67.31 0)
					(length 3.81)
					(name "TXRX4_D_P")
					(number "42")
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 3.81)
					(name "TXRX4_D_N")
					(number "43")
				)
				(pin bidirectional line
					(at 30.48 -6.35 180)
					(length 3.81)
					(name "TX_CLK6")
					(number "48")
					(alternate "REFCLKI6" passive line)
				)
				(pin input line
					(at 30.48 -8.89 180)
					(length 3.81)
					(name "TX_EN6")
					(number "49")
					(alternate "TX_CTL6" passive line)
				)
				(pin input line
					(at 30.48 -11.43 180)
					(length 3.81)
					(name "TX_ER6")
					(number "50")
				)
				(pin bidirectional line
					(at 30.48 0 180)
					(length 3.81)
					(name "COL6")
					(number "51")
				)
				(pin output line
					(at 30.48 -21.59 180)
					(length 3.81)
					(name "TXD6_3")
					(number "52")
				)
				(pin output line
					(at 30.48 -19.05 180)
					(length 3.81)
					(name "TXD6_2")
					(number "53")
				)
				(pin output line
					(at 30.48 -16.51 180)
					(length 3.81)
					(name "TXD6_1")
					(number "54")
				)
				(pin output line
					(at 30.48 -13.97 180)
					(length 3.81)
					(name "TXD6_0")
					(number "55")
				)
				(pin bidirectional line
					(at 30.48 -25.4 180)
					(length 3.81)
					(name "RX_CLK6")
					(number "57")
					(alternate "REFCLKO6" passive line)
				)
				(pin output line
					(at 30.48 -27.94 180)
					(length 3.81)
					(name "RX_DV6")
					(number "58")
					(alternate "CRS_DV6" passive line)
					(alternate "RX_CTL6" passive line)
				)
				(pin output line
					(at 30.48 -30.48 180)
					(length 3.81)
					(name "RX_ER6")
					(number "59")
				)
				(pin bidirectional line
					(at 30.48 -2.54 180)
					(length 3.81)
					(name "CRS6")
					(number "60")
				)
				(pin input line
					(at 30.48 -40.64 180)
					(length 3.81)
					(name "RXD6_3")
					(number "62")
				)
				(pin input line
					(at 30.48 -38.1 180)
					(length 3.81)
					(name "RXD6_2")
					(number "63")
				)
				(pin input line
					(at 30.48 -35.56 180)
					(length 3.81)
					(name "RXD6_1")
					(number "64")
				)
				(pin input line
					(at 30.48 -33.02 180)
					(length 3.81)
					(name "RXD6_0")
					(number "65")
				)
				(pin input line
					(at 30.48 -54.61 180)
					(length 3.81)
					(name "S_REXT")
					(number "76")
				)
				(pin input line
					(at 30.48 -46.99 180)
					(length 3.81)
					(name "S_IN7_N")
					(number "78")
				)
				(pin input line
					(at 30.48 -44.45 180)
					(length 3.81)
					(name "S_IN7_P")
					(number "79")
				)
				(pin output line
					(at 30.48 -49.53 180)
					(length 3.81)
					(name "S_OUT7_P")
					(number "81")
				)
				(pin output line
					(at 30.48 -52.07 180)
					(length 3.81)
					(name "S_OUT7_N")
					(number "82")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 3.81)
					(name "TXRX5_A_P")
					(number "112")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 3.81)
					(name "TXRX5_A_N")
					(number "113")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 3.81)
					(name "TXRX5_B_P")
					(number "115")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 3.81)
					(name "TXRX5_B_N")
					(number "116")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 3.81)
					(name "TXRX5_C_P")
					(number "117")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 3.81)
					(name "TXRX5_C_N")
					(number "118")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 3.81)
					(name "TXRX5_D_P")
					(number "120")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 3.81)
					(name "TXRX5_D_N")
					(number "121")
				)
			)
			(embedded_fonts no)
		)
)
