(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "KTS1682EAY"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "KTS1682EAY"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "KTS1682EAY"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/936/KTS1682_04b-1634491.pdf"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Power Switch 4.5 AMP 38MOHM OVERVOLTAGE PROTECTION"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Kinetic Technologies"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "KTS1682EAY-TR"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "POWER, SWITCH, SMT, PMIC, IC, VOLTAGE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "KTS1682EAY_1_1"
				(pin input line
					(at 20.32 -10.16 180)
					(length 2.54)
					(name "CTRL")
					(number "A1")
				)
				(pin power_out line
					(at 20.32 0 180)
					(length 2.54)
					(name "OUT")
					(number "A2")
				)
				(pin passive line
					(at 20.32 0 180)
					(length 2.54)
					(hide yes)
					(name "OUT")
					(number "A3")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "GND")
					(number "A4")
				)
				(pin output line
					(at 20.32 -5.08 180)
					(length 2.54)
					(name "VDET")
					(number "B1")
				)
				(pin passive line
					(at 20.32 0 180)
					(length 2.54)
					(hide yes)
					(name "OUT")
					(number "B2")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "IN")
					(number "B3")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "B4")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "OVLO")
					(number "C1")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "IN")
					(number "C2")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "IN")
					(number "C3")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "C4")
				)
			)
			(embedded_fonts no)
		)
)
