(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LM5148PSQRGYRQ1"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LM5148PSQRGYRQ1"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LM5148PSQRGYRQ1"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm5148-q1.pdf"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Automotive, 80V synchronous buck DC/DC controller with ultra-low IQ"
				(at 35.56 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LM5148PSQRGYRQ1"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, SWITCHING, BUCK, VOLTAGE, REGULATOR"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "VQFN24_RGY_TEX VQFN24_RGY_TEX-M VQFN24_RGY_TEX-L"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LM5148PSQRGYRQ1_1_1"
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "CNFG")
					(number "1")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(name "RT")
					(number "2")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(name "EXTCOMP")
					(number "3")
				)
				(pin input line
					(at 22.86 -25.4 180)
					(length 2.54)
					(name "FB")
					(number "4")
				)
				(pin power_in line
					(at 0 -33.02 0)
					(length 2.54)
					(name "AGND")
					(number "5")
				)
				(pin passive line
					(at 22.86 0 180)
					(length 2.54)
					(name "VDDA")
					(number "6")
				)
				(pin power_out line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VCC")
					(number "7")
				)
				(pin power_in line
					(at 22.86 -33.02 180)
					(length 2.54)
					(name "PGND")
					(number "8")
				)
				(pin passive line
					(at 22.86 -15.24 180)
					(length 2.54)
					(name "LO")
					(number "9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VIN")
					(number "10")
				)
				(pin passive line
					(at 22.86 -10.16 180)
					(length 2.54)
					(name "HO")
					(number "11")
				)
				(pin passive line
					(at 22.86 -12.7 180)
					(length 2.54)
					(name "SW")
					(number "12")
				)
				(pin passive line
					(at 22.86 -5.08 180)
					(length 2.54)
					(name "CBOOT")
					(number "13")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VCCX")
					(number "14")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "PG")
					(number "15")
					(alternate "SYNCOUT" passive line)
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "PFM")
					(number "16")
					(alternate "SYNC" passive line)
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "EN")
					(number "17")
				)
				(pin input line
					(at 22.86 -20.32 180)
					(length 2.54)
					(name "ISNS+")
					(number "18")
				)
				(pin input line
					(at 22.86 -22.86 180)
					(length 2.54)
					(name "VOUT")
					(number "19")
				)
				(pin power_in line
					(at 22.86 -30.48 180)
					(length 2.54)
					(name "EP")
					(number "20")
				)
			)
			(embedded_fonts no)
		)
)
