(footprint "VQFN-24-1EP_3.5x5.5x1mm_P0.5mm_EP2.1x4.1mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Layout according to https://www.ti.com/lit/ds/symlink/lm5148-q1.pdf")
	(property "Reference" "REF**"
		(at -1.2 -3.5 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "VQFN-24-1EP_3.5x5.5x1mm_P0.5mm_EP2.1x4.1mm"
		(at -2.6 4.5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd allow_soldermask_bridges)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -2.6 5.7 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -2.6 6.8 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -2.6 8 0)
		(layer "F.Fab")
	)
	(fp_text user ""
		(at 0 -4 0)
		(unlocked yes)
		(layer "User.5")
	)
	(fp_text user ""
		(at 0 -2.5 0)
		(unlocked yes)
		(layer "User.9")
	)
	(pad "" smd roundrect
		(at -0.55 -1.35)
		(size 0.94 1.16)
		(layers "F.Paste")
		(roundrect_rratio 0.02873563218)
	)
	(pad "" smd roundrect
		(at -0.55 0)
		(size 0.94 1.16)
		(layers "F.Paste")
		(roundrect_rratio 0.02873563218)
	)
	(pad "" smd roundrect
		(at -0.55 1.35)
		(size 0.94 1.16)
		(layers "F.Paste")
		(roundrect_rratio 0.02873563218)
	)
	(pad "" smd roundrect
		(at 0.55 -1.35)
		(size 0.94 1.16)
		(layers "F.Paste")
		(roundrect_rratio 0.02873563218)
	)
	(pad "" smd roundrect
		(at 0.55 0)
		(size 0.94 1.16)
		(layers "F.Paste")
		(roundrect_rratio 0.02873563218)
	)
	(pad "" smd roundrect
		(at 0.55 1.35)
		(size 0.94 1.16)
		(layers "F.Paste")
		(roundrect_rratio 0.02873563218)
	)
	(pad "1" smd roundrect
		(at -0.75 -2.7)
		(size 0.254 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -1.7 -2.25 90)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.7 -1.75 90)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.7 -1.25 90)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -1.7 -0.75 90)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -1.7 -0.25 90)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -1.7 0.25 90)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -1.7 0.75 90)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -1.7 1.25 90)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -1.7 1.75 90)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -1.7 2.25 90)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -0.75 2.7)
		(size 0.254 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 0.75 2.7)
		(size 0.254 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 1.7 2.25 90)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at 1.7 1.75 90)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at 1.7 1.25 90)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at 1.7 0.75 90)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at 1.7 0.25 90)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at 1.7 -0.25 90)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 1.7 -0.75 90)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 1.7 -1.25 90)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at 1.7 -1.75 90)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at 1.7 -2.25 90)
		(size 0.25 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at 0.75 -2.7)
		(size 0.254 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at 0 0)
		(size 2.1 4.1)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.03)
	)
	(embedded_fonts no)
	(model "antmicro_lm5148qrgyrq1.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
