(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LM73605RNPT"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LM73605RNPT"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LM73605RNPT"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm73605.pdf?ts=1721914948836"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Switching Voltage Regulators 3.5V to 36V,5A Synch Step-Down VConverter"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 38.1 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LM73605RNPT"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, VOLTAGE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LM73605RNPT_1_1"
				(pin passive line
					(at 22.86 0 180)
					(length 2.54)
					(name "SW")
					(number "1")
				)
				(pin passive line
					(at 22.86 0 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "2")
				)
				(pin passive line
					(at 22.86 0 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "3")
				)
				(pin passive line
					(at 22.86 0 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "4")
				)
				(pin passive line
					(at 22.86 0 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "5")
				)
				(pin passive line
					(at 22.86 -5.08 180)
					(length 2.54)
					(name "CBOOT")
					(number "6")
				)
				(pin power_out line
					(at 22.86 -25.4 180)
					(length 2.54)
					(name "VCC")
					(number "7")
				)
				(pin passive line
					(at 22.86 -10.16 180)
					(length 2.54)
					(name "BIAS")
					(number "8")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "RT")
					(number "9")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "SS/TRK")
					(number "10")
				)
				(pin input line
					(at 22.86 -15.24 180)
					(length 2.54)
					(name "FB")
					(number "11")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "12")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "13")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "14")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "15")
				)
				(pin output line
					(at 22.86 -20.32 180)
					(length 2.54)
					(name "PGOOD")
					(number "16")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "SYNC/MODE")
					(number "17")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "EN")
					(number "18")
				)
				(pin power_in line
					(at 0 -25.4 0)
					(length 2.54)
					(name "GND")
					(number "19")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "PVIN")
					(number "20")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "PVIN")
					(number "21")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "PVIN")
					(number "22")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "23")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "24")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "25")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "26")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "27")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "28")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "29")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "30")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "31")
				)
			)
			(embedded_fonts no)
		)
)
