(footprint "VQFN-HR-14_3.5x4mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -2.41 0)
		(layer "F.SilkS")
	)
	(property "Value" "VQFN-HR-14_3.5x4mm"
		(at 0 3.18 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -4.33 5.18 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -4.33 6.38 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -4.33 7.58 0)
		(layer "F.Fab")
	)
	(pad "1" smd custom
		(at -1.68 -1.45)
		(size 0.36 1.01)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.075)
		(solder_paste_margin -0.04)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.17 0.5) (xy -0.52 0.5) (xy -0.52 0.1) (xy 0.17 0.1)
				)
				(width 0.02)
				(fill yes)
			)
		)
	)
	(pad "2" smd roundrect
		(at -1.855 -0.527)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.06)
		(solder_mask_margin 0.075)
	)
	(pad "3" smd roundrect
		(at -1.855 0)
		(size 0.7 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.07)
		(solder_mask_margin 0.075)
	)
	(pad "4" smd roundrect
		(at -1.855 0.525)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.06)
		(solder_mask_margin 0.075)
	)
	(pad "5" smd custom
		(at -1.68 1.449 180)
		(size 0.36 1.01)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.075)
		(solder_paste_margin -0.04)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.17 0.5) (xy 0.52 0.5) (xy 0.52 0.1) (xy -0.17 0.1)
				)
				(width 0.02)
				(fill yes)
			)
		)
	)
	(pad "6" smd roundrect
		(at -1.131 1.6 90)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.06)
		(solder_mask_margin 0.075)
	)
	(pad "7" smd roundrect
		(at -0.63 1.6 90)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.06)
		(solder_mask_margin 0.075)
	)
	(pad "8" smd roundrect
		(at 0.444 1.449 90)
		(size 1 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(solder_mask_margin 0.075)
	)
	(pad "9" smd custom
		(at 1.594 1.449 180)
		(size 0.4 1.01)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.075)
		(solder_paste_margin -0.04)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.17 0.5) (xy -0.6 0.5) (xy -0.6 0.1) (xy 0.17 0.1)
				)
				(width 0.02)
				(fill yes)
			)
		)
	)
	(pad "10" smd roundrect
		(at 0.994 0)
		(size 2.4 0.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
		(solder_mask_margin 0.075)
	)
	(pad "11" smd custom
		(at 1.594 -1.45)
		(size 0.4 1.01)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.075)
		(solder_paste_margin -0.04)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.17 0.5) (xy 0.6 0.5) (xy 0.6 0.1) (xy -0.17 0.1)
				)
				(width 0.02)
				(fill yes)
			)
		)
	)
	(pad "12" smd roundrect
		(at 0.444 -1.45 90)
		(size 1 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(solder_mask_margin 0.075)
	)
	(pad "13" smd roundrect
		(at -0.63 -1.601 90)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.06)
		(solder_mask_margin 0.075)
	)
	(pad "14" smd roundrect
		(at -1.131 -1.601 90)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.06)
		(solder_mask_margin 0.075)
	)
	(embedded_fonts no)
	(model "antmicro_lmq62440bppqrjrrq1.glb"
		(offset
			(xyz -0.005 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
