(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LMR51460SQDRRRQ1"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 30.48 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LMR51460SQDRRRQ1"
				(at 30.48 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LMR51460SQDRRRQ1"
				(at 30.48 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lmr51460-q1.pdf"
				(at 30.48 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Switching Voltage Regulators Automotive 36V 6A Synchronous Buck Converter"
				(at 30.48 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LMR51460SQDRRRQ1"
				(at 30.48 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 30.48 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 30.48 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 30.48 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, VOLTAGE, DC-DC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LMR51460SQDRRRQ1_1_1"
				(pin power_out line
					(at 19.05 -5.08 180)
					(length 2.54)
					(name "SW")
					(number "1")
				)
				(pin passive line
					(at 19.05 -5.08 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "2")
				)
				(pin passive line
					(at 19.05 -5.08 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "3")
				)
				(pin input line
					(at 19.05 0 180)
					(length 2.54)
					(name "BOOT")
					(number "4")
				)
				(pin output line
					(at 19.05 -15.24 180)
					(length 2.54)
					(name "PG")
					(number "5")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "RT/SYNC")
					(number "6")
				)
				(pin input line
					(at 19.05 -10.16 180)
					(length 2.54)
					(name "FB")
					(number "7")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "GND")
					(number "8")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "EN")
					(number "9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VIN")
					(number "10")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VIN")
					(number "11")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VIN")
					(number "12")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "13")
				)
			)
			(embedded_fonts no)
		)
)
