(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LT1461CCS8-5"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LT1461CCS8-5"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LT1461CCS8-5"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/609/LT1461-3123288.pdf"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Voltage reference, micropower, precision, low dropout series"
				(at 33.02 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LT1461CCS8-5#TRPBF"
				(at 33.02 -8.255 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Analog Devices"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, POWER, SWITCH, DRIVER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LT1461CCS8-5_1_1"
				(pin no_connect line
					(at 13.97 -1.27 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "1")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "IN")
					(number "2")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "~{SHDN}")
					(number "3")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "GND")
					(number "4")
				)
				(pin no_connect line
					(at 13.97 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "5")
				)
				(pin output line
					(at 16.51 0 180)
					(length 2.54)
					(name "OUT")
					(number "6")
				)
				(pin no_connect line
					(at 13.97 -3.81 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "7")
				)
				(pin no_connect line
					(at 13.97 -5.08 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
