(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LT1976EFE"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 36.83 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LT1976EFE"
				(at 36.83 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LT1976EFE"
				(at 36.83 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/609/1976bfg-1268881.pdf"
				(at 36.83 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Switching voltage regulator Hi V 1.5A, 200kHz Buck Sw Reg w/ 100 A"
				(at 36.83 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LT1976EFE#TRPBF"
				(at 36.83 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Analog Devices"
				(at 36.83 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 36.83 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 36.83 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "BUCK, SWITCHING, REGULATOR, DC-DC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "TSOT?23*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LT1976EFE_1_1"
				(pin no_connect line
					(at 0 -10.16 0)
					(length 2.54)
					(name "NC")
					(number "1")
				)
				(pin power_out line
					(at 17.78 -5.08 180)
					(length 2.54)
					(name "SW")
					(number "2")
				)
				(pin no_connect line
					(at 0 -11.43 0)
					(length 2.54)
					(name "NC")
					(number "3")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{IN}")
					(number "4")
				)
				(pin no_connect line
					(at 0 -12.7 0)
					(length 2.54)
					(name "NC")
					(number "5")
				)
				(pin input line
					(at 17.78 0 180)
					(length 2.54)
					(name "BOOST")
					(number "6")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "C_{T}")
					(number "7")
				)
				(pin power_in line
					(at 0 -22.86 0)
					(length 2.54)
					(name "GND")
					(number "8")
				)
				(pin passive line
					(at 17.78 -8.89 180)
					(length 2.54)
					(name "C_{SS}")
					(number "9")
				)
				(pin input line
					(at 17.78 -12.7 180)
					(length 2.54)
					(name "V_{BIAS}")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "V_{C}")
					(number "11")
				)
				(pin input line
					(at 17.78 -17.78 180)
					(length 2.54)
					(name "FB")
					(number "12")
				)
				(pin input line
					(at 17.78 -20.32 180)
					(length 2.54)
					(name "PGFB")
					(number "13")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "SYNC")
					(number "14")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "~{SHDN}")
					(number "15")
				)
				(pin output line
					(at 17.78 -22.86 180)
					(length 2.54)
					(name "PG")
					(number "16")
				)
			)
			(embedded_fonts no)
		)
)
