(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LT3507AEFE"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LT3507AEFE"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LT3507AEFE"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/609/3507afa-2954803.pdf"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Triple Monolithic Step-Down Regulator with LDO"
				(at 45.72 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LT3507AEFE#PBF"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Analog Devices"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "BUCK, SWITCHING, REGULATOR, DC-DC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LT3507AEFE_1_1"
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VIN3")
					(number "1")
				)
				(pin output line
					(at 24.13 -11.43 180)
					(length 2.54)
					(name "SW1")
					(number "2")
				)
				(pin passive line
					(at 24.13 -11.43 180)
					(length 2.54)
					(name "SW1")
					(number "3")
				)
				(pin input line
					(at 24.13 -8.89 180)
					(length 2.54)
					(name "BOOST1")
					(number "4")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VIN1")
					(number "5")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "VIN1")
					(number "6")
				)
				(pin output line
					(at 0 -19.05 0)
					(length 2.54)
					(name "VINSW")
					(number "7")
				)
				(pin input line
					(at 0 -21.59 0)
					(length 2.54)
					(name "OVLO")
					(number "8")
				)
				(pin input line
					(at 0 -24.13 0)
					(length 2.54)
					(name "UVLO")
					(number "9")
				)
				(pin output line
					(at 24.13 -16.51 180)
					(length 2.54)
					(name "VC1")
					(number "10")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "TRK-SS1")
					(number "11")
					(alternate "SS1" passive line)
				)
				(pin input line
					(at 24.13 -13.97 180)
					(length 2.54)
					(name "FB1")
					(number "12")
				)
				(pin open_collector line
					(at 24.13 0 180)
					(length 2.54)
					(name "PG0OD1")
					(number "13")
				)
				(pin open_collector line
					(at 24.13 -2.54 180)
					(length 2.54)
					(name "PG0OD2")
					(number "14")
				)
				(pin open_collector line
					(at 24.13 -5.08 180)
					(length 2.54)
					(name "PG0OD3")
					(number "15")
				)
				(pin input line
					(at 0 -46.99 0)
					(length 2.54)
					(name "RT")
					(number "16")
					(alternate "SYNC" passive line)
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "RUN1")
					(number "17")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "RUN2")
					(number "18")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "RUN3")
					(number "19")
				)
				(pin power_in line
					(at 0 -52.07 0)
					(length 2.54)
					(name "GND")
					(number "20")
				)
				(pin input line
					(at 24.13 -46.99 180)
					(length 2.54)
					(name "BIAS")
					(number "21")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "TRK-SS3")
					(number "22")
				)
				(pin output line
					(at 24.13 -41.91 180)
					(length 2.54)
					(name "VC3")
					(number "23")
				)
				(pin input line
					(at 24.13 -39.37 180)
					(length 2.54)
					(name "FB3")
					(number "24")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "TRK-SS2")
					(number "25")
				)
				(pin input line
					(at 24.13 -26.67 180)
					(length 2.54)
					(name "FB2")
					(number "26")
				)
				(pin no_connect line
					(at 2.54 -40.64 0)
					(length 2.54)
					(name "NC")
					(number "27")
				)
				(pin output line
					(at 24.13 -29.21 180)
					(length 2.54)
					(name "VC2")
					(number "28")
				)
				(pin output line
					(at 24.13 -49.53 180)
					(length 2.54)
					(name "DRIVE")
					(number "29")
				)
				(pin input line
					(at 24.13 -52.07 180)
					(length 2.54)
					(name "FB4")
					(number "30")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "TRK-SS4")
					(number "31")
				)
				(pin input line
					(at 24.13 -21.59 180)
					(length 2.54)
					(name "BOOST2")
					(number "32")
				)
				(pin output line
					(at 24.13 -24.13 180)
					(length 2.54)
					(name "SW2")
					(number "33")
				)
				(pin no_connect line
					(at 2.54 -39.37 0)
					(length 2.54)
					(name "NC")
					(number "34")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VIN2")
					(number "35")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VIN2")
					(number "36")
				)
				(pin input line
					(at 24.13 -34.29 180)
					(length 2.54)
					(name "BOOST3")
					(number "37")
				)
				(pin output line
					(at 24.13 -36.83 180)
					(length 2.54)
					(name "SW3")
					(number "38")
				)
				(pin power_in line
					(at 0 -49.53 0)
					(length 2.54)
					(name "EP")
					(number "39")
				)
			)
			(embedded_fonts no)
		)
)
