(footprint "DFN-12-1EP_4x3mm_P0.5mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Reference LTC DWG # 05-08-1695 Rev D")
	(property "Reference" "REF**"
		(at -2.3 -2.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "DFN-12-1EP_4x3mm_P0.5mm"
		(at -3.1 3.175 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -3.1 5.175 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -3.1 6.375 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -3.1 7.575 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -1.45 -1.25)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "2" smd roundrect
		(at -1.45 -0.75)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "3" smd roundrect
		(at -1.45 -0.25)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "4" smd roundrect
		(at -1.45 0.25)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "5" smd roundrect
		(at -1.45 0.75)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "6" smd roundrect
		(at -1.45 1.25)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "7" smd roundrect
		(at 1.45 1.25)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "8" smd roundrect
		(at 1.45 0.75)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "9" smd roundrect
		(at 1.45 0.25)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "10" smd roundrect
		(at 1.45 -0.25)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "11" smd roundrect
		(at 1.45 -0.75)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "12" smd roundrect
		(at 1.45 -1.25)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "13" smd roundrect
		(at 0 0)
		(size 1.7 3.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(chamfer_ratio 0.1176470588)
		(chamfer top_left)
	)
	(embedded_fonts no)
	(model "antmicro_ltc2855hde_pbf.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 -90)
		)
	)
)
