(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LTC2855HDE"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 39.37 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LTC2855HDE"
				(at 39.37 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LTC2855HDE"
				(at 39.37 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/285455fc.pdf"
				(at 39.37 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "3.3V 20Mbps RS485/RS422 Transceiver with Integrated Switchable Termination"
				(at 39.37 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LTC2855HDE#PBF"
				(at 39.37 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Analog Devices"
				(at 39.37 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 39.37 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 39.37 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, IC, DRIVER, TRANSCEIVER"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LTC2855HDE_1_1"
				(text "125k"
					(at 14.605 -5.08 900)
				)
				(text "125k"
					(at 14.732 0 900)
				)
				(text "120R"
					(at 17.145 0 900)
				)
				(pin output line
					(at 0 -2.54 0)
					(length 2.54)
					(name "RO")
					(number "1")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "~{RE}")
					(number "2")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "DE")
					(number "3")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "DI")
					(number "4")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "TE")
					(number "5")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "GND")
					(number "6")
				)
				(pin no_connect line
					(at 22.86 -7.62 180)
					(length 2.54)
					(name "NC")
					(number "7")
				)
				(pin bidirectional line
					(at 25.4 -15.24 180)
					(length 2.54)
					(name "Y")
					(number "8")
				)
				(pin bidirectional line
					(at 25.4 -12.7 180)
					(length 2.54)
					(name "Z")
					(number "9")
				)
				(pin bidirectional line
					(at 25.4 -2.54 180)
					(length 2.54)
					(name "B")
					(number "10")
				)
				(pin bidirectional line
					(at 25.4 0 180)
					(length 2.54)
					(name "A")
					(number "11")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{CC}")
					(number "12")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "GND")
					(number "13")
				)
			)
			(embedded_fonts no)
		)
)
