(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LTC3311S"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 39.37 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LTC3311S"
				(at 39.37 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LTC3311S"
				(at 39.37 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ltc3311s.pdf"
				(at 39.37 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "DC/DC Switching Regulator, 12.5A, 5.5V Synchr SS1 Buck Regulator"
				(at 39.37 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Analog Devices"
				(at 39.37 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LTC3311SIV#PBF "
				(at 39.37 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 39.37 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 39.37 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, SWITCHING, BUCK, VOLTAGE, REGULATOR"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LTC3311S_1_0"
				(pin power_in line
					(at 0 -17.78 0)
					(length 2.54)
					(hide yes)
					(name "PGND")
					(number "10")
				)
			)
			(symbol "LTC3311S_1_1"
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "EN")
					(number "1")
				)
				(pin input line
					(at 22.86 -12.7 180)
					(length 2.54)
					(name "AGND")
					(number "2")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VIN")
					(number "3")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VIN")
					(number "4")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 2.54)
					(name "PGND")
					(number "5")
				)
				(pin power_out line
					(at 22.86 -2.54 180)
					(length 2.54)
					(name "SW")
					(number "6")
				)
				(pin power_out line
					(at 22.86 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "7")
				)
				(pin power_out line
					(at 22.86 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "8")
				)
				(pin power_out line
					(at 22.86 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VIN")
					(number "11")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VIN")
					(number "12")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "MODE/SYNC")
					(number "13")
				)
				(pin open_collector line
					(at 22.86 0 180)
					(length 2.54)
					(name "PGOOD")
					(number "14")
				)
				(pin passive line
					(at 22.86 -17.78 180)
					(length 2.54)
					(name "RT")
					(number "15")
				)
				(pin output line
					(at 0 -10.16 0)
					(length 2.54)
					(name "SSTT")
					(number "16")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "ITH")
					(number "17")
				)
				(pin input line
					(at 22.86 -7.62 180)
					(length 2.54)
					(name "FB")
					(number "18")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 2.54)
					(hide yes)
					(name "PGND")
					(number "19")
				)
			)
			(embedded_fonts no)
		)
)
