(footprint "SOIC-8-1EP_3.9x4.9x1.75mm_P1.27mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(tags "Integrated Circuit")
	(property "Reference" "REF**"
		(at 0 -2.849 0)
		(layer "F.SilkS")
	)
	(property "Value" "SOIC-8-1EP_3.9x4.9x1.75mm_P1.27mm"
		(at 0 3.651 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -3.6 5.651 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -3.6 6.851 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -3.6 8.051 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -2.715 -1.905 90)
		(size 0.65 1.525)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.715 -0.635 90)
		(size 0.65 1.525)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -2.715 0.635 90)
		(size 0.65 1.525)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -2.715 1.905 90)
		(size 0.65 1.525)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 2.71 1.905 90)
		(size 0.65 1.525)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 2.71 0.635 90)
		(size 0.65 1.525)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 2.71 -0.635 90)
		(size 0.65 1.525)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 2.71 -1.905 90)
		(size 0.65 1.525)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 0 0)
		(size 2.29 3.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_lv14540ddar.glb"
		(offset
			(xyz 0 -0.001 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
