(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LV14540DDAR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LV14540DDAR"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LV14540DDAR"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lv14540.pdf?ts=1711947439079&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FLV14540%253FkeyMatch%253DLV14540%2526tisearch%253Dsearch-everything%2526usecase%253DGPN"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Step-Down Converter, 40V, 5A, 2MHz"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LV14540DDAR "
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, VOLTAGE, REGULATOR, DC-DC,BUCK,SWITCHING,SMT"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LV14540DDAR_1_1"
				(pin input line
					(at 17.78 0 180)
					(length 2.54)
					(name "BOOT")
					(number "1")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VIN")
					(number "2")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "EN")
					(number "3")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "RT")
					(number "4")
					(alternate "WYNC" passive line)
				)
				(pin input line
					(at 17.78 -15.24 180)
					(length 2.54)
					(name "FB")
					(number "5")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SS")
					(number "6")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "GND")
					(number "7")
				)
				(pin power_out line
					(at 17.78 -7.62 180)
					(length 2.54)
					(name "SW")
					(number "8")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "EP")
					(number "9")
				)
			)
			(embedded_fonts no)
		)
)
