(footprint "TQFN-20-1EP_5x5mm_P0.65mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -3 -3.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "TQFN-20-1EP_5x5mm_P0.65mm"
		(at -3.3 4.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -3.3 5.6 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -3.3 6.8 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -3.3 8 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -2.34 -1.3)
		(size 0.99 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "2" smd roundrect
		(at -2.34 -0.65)
		(size 0.99 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "3" smd roundrect
		(at -2.34 0)
		(size 0.99 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "4" smd roundrect
		(at -2.34 0.65)
		(size 0.99 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "5" smd roundrect
		(at -2.34 1.3)
		(size 0.99 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "6" smd roundrect
		(at -1.3 2.34 90)
		(size 0.99 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "7" smd roundrect
		(at -0.65 2.34 90)
		(size 0.99 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "8" smd roundrect
		(at 0 2.34 90)
		(size 0.99 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "9" smd roundrect
		(at 0.65 2.34 90)
		(size 0.99 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "10" smd roundrect
		(at 1.3 2.34 90)
		(size 0.99 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "11" smd roundrect
		(at 2.34 1.3)
		(size 0.99 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "12" smd roundrect
		(at 2.34 0.65)
		(size 0.99 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "13" smd roundrect
		(at 2.34 0)
		(size 0.99 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "14" smd roundrect
		(at 2.34 -0.65)
		(size 0.99 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "15" smd roundrect
		(at 2.34 -1.3)
		(size 0.99 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "16" smd roundrect
		(at 1.3 -2.34 90)
		(size 0.99 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "17" smd roundrect
		(at 0.65 -2.34 90)
		(size 0.99 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "18" smd roundrect
		(at 0 -2.34 90)
		(size 0.99 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "19" smd roundrect
		(at -0.65 -2.34 90)
		(size 0.99 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "20" smd roundrect
		(at -1.3 -2.34 90)
		(size 0.99 0.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "21" smd rect
		(at 0 0)
		(size 3.15 3.15)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "antmicro_max16922atph_v.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
