(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MAX16922ATPH_V+"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -1.27 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MAX16922ATPH_V+"
				(at 35.56 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MAX16922ATPH_V+"
				(at 35.56 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/max16922.pdf"
				(at 35.56 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "2.2MHz, Dual, Step-Down DC-DC Converters, Dual LDOs, and RESET"
				(at 35.56 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MAX16922ATPH/V+"
				(at 35.56 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Analog Devices"
				(at 35.56 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, VOLTAGE, REGULATOR, SWITCHING, DC-DC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MAX16922ATPH_V+_0_0"
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "PV1")
					(number "2")
				)
				(pin output line
					(at 17.78 -13.97 180)
					(length 2.54)
					(name "LX1")
					(number "3")
				)
				(pin input line
					(at 17.78 -16.51 180)
					(length 2.54)
					(name "OUTS1")
					(number "5")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "PWM")
					(number "6")
				)
				(pin input line
					(at 17.78 0 180)
					(length 2.54)
					(name "OUTS2")
					(number "8")
				)
				(pin power_in line
					(at 17.78 -5.08 180)
					(length 2.54)
					(name "PGND2")
					(number "9")
				)
				(pin output line
					(at 17.78 -2.54 180)
					(length 2.54)
					(name "LX2")
					(number "10")
				)
				(pin power_in line
					(at 17.78 -8.89 180)
					(length 2.54)
					(name "PV2")
					(number "11")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "PV3")
					(number "12")
				)
				(pin output line
					(at 0 -12.7 0)
					(length 2.54)
					(name "OUT3")
					(number "13")
				)
				(pin output line
					(at 0 -17.78 0)
					(length 2.54)
					(name "OUT4")
					(number "15")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "PV4")
					(number "16")
				)
				(pin input line
					(at 17.78 -22.86 180)
					(length 2.54)
					(name "LSUP")
					(number "17")
				)
				(pin output line
					(at 0 0 0)
					(length 2.54)
					(name "~{RESET}")
					(number "18")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "EN")
					(number "20")
				)
			)
			(symbol "MAX16922ATPH_V+_1_0"
				(pin passive line
					(at 17.78 -11.43 180)
					(length 2.54)
					(name "BST")
					(number "1")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "4")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "7")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "14")
				)
				(pin power_in line
					(at 0 -22.86 0)
					(length 2.54)
					(name "GND")
					(number "19")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 2.54)
					(name "EP")
					(number "21")
				)
			)
			(embedded_fonts no)
		)
)
