(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MAX1708EEE+"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 30.48 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MAX1708EEE+"
				(at 30.48 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MAX1708EEE+"
				(at 30.48 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX1708.pdf"
				(at 30.48 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Step Up Regulator,  700mV-5V in, 3.3V-5V/2A out, QSOP-16"
				(at 30.48 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MAX1708EEE+"
				(at 30.48 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Maxim Integrated Products"
				(at 30.48 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 30.48 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 30.48 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, VOLTAGE, REGULATOR, SWITCHING, DC-DC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "MAX1708EEE"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MAX1708EEE+_1_1"
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "~{ONB}")
					(number "1")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "ONA")
					(number "2")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "LX")
					(number "3")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "LX")
					(number "4")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "LX")
					(number "5")
				)
				(pin passive line
					(at 20.32 -15.24 180)
					(length 2.54)
					(name "GND")
					(number "6")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "SS/LIM")
					(number "7")
				)
				(pin output line
					(at 0 -17.78 0)
					(length 2.54)
					(name "REF")
					(number "8")
				)
				(pin passive line
					(at 20.32 -15.24 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "9")
				)
				(pin input line
					(at 20.32 0 180)
					(length 2.54)
					(name "OUT")
					(number "10")
				)
				(pin input line
					(at 20.32 -11.43 180)
					(length 2.54)
					(name "FB")
					(number "11")
				)
				(pin passive line
					(at 20.32 -17.78 180)
					(length 2.54)
					(name "PGND")
					(number "12")
				)
				(pin passive line
					(at 20.32 -17.78 180)
					(length 2.54)
					(hide yes)
					(name "PGND")
					(number "13")
				)
				(pin passive line
					(at 20.32 -17.78 180)
					(length 2.54)
					(hide yes)
					(name "PGND")
					(number "14")
				)
				(pin input line
					(at 20.32 -3.81 180)
					(length 2.54)
					(name "~{3.3}/5")
					(number "15")
				)
				(pin input line
					(at 20.32 -7.62 180)
					(length 2.54)
					(name "CLK")
					(number "16")
				)
			)
			(embedded_fonts no)
		)
)
