(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MAX20029ATIA_V+"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 36.83 -1.27 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MAX20029ATIA_V+"
				(at 36.83 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MAX20029ATIA_V+"
				(at 36.83 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/en/products/max20029.html"
				(at 36.83 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Automotive Quad/Triple Low-Voltage Step-Down DC-DC Converter"
				(at 36.83 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MAX20029ATIA/V+"
				(at 36.83 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Analog Devices"
				(at 36.83 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 36.83 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 36.83 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, SWITCHING, VOLTAGE, REGULATOR, DC-DC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MAX20029ATIA_V+_1_1"
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "EN1")
					(number "1")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "PV1")
					(number "2")
				)
				(pin power_out line
					(at 25.4 -7.62 180)
					(length 2.54)
					(name "LX1")
					(number "3")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 2.54)
					(name "PGND1")
					(number "4")
				)
				(pin power_in line
					(at 0 -22.86 0)
					(length 2.54)
					(name "PGND2")
					(number "5")
				)
				(pin power_out line
					(at 25.4 -17.78 180)
					(length 2.54)
					(name "LX2")
					(number "6")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 2.54)
					(name "PV2")
					(number "7")
				)
				(pin passive line
					(at 25.4 -20.32 180)
					(length 2.54)
					(name "OUTS2")
					(number "8")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "EN2")
					(number "9")
				)
				(pin output line
					(at 25.4 -22.86 180)
					(length 2.54)
					(name "PG2")
					(number "10")
				)
				(pin power_in line
					(at 0 -48.26 0)
					(length 2.54)
					(name "GND")
					(number "11")
				)
				(pin output line
					(at 25.4 -33.02 180)
					(length 2.54)
					(name "PG3")
					(number "12")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "EN3")
					(number "13")
				)
				(pin passive line
					(at 25.4 -40.64 180)
					(length 2.54)
					(name "OUTS3")
					(number "14")
				)
				(pin power_in line
					(at 0 -27.94 0)
					(length 2.54)
					(name "PV3")
					(number "15")
				)
				(pin power_out line
					(at 25.4 -38.1 180)
					(length 2.54)
					(name "LX3")
					(number "16")
				)
				(pin power_in line
					(at 0 -33.02 0)
					(length 2.54)
					(name "PGND3")
					(number "17")
				)
				(pin power_in line
					(at 0 -43.18 0)
					(length 2.54)
					(name "PGND4")
					(number "18")
				)
				(pin power_out line
					(at 25.4 -27.94 180)
					(length 2.54)
					(name "LX4")
					(number "19")
				)
				(pin power_in line
					(at 0 -38.1 0)
					(length 2.54)
					(name "PV4")
					(number "20")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 2.54)
					(name "EN4")
					(number "21")
				)
				(pin passive line
					(at 25.4 -30.48 180)
					(length 2.54)
					(name "OUTS4")
					(number "22")
				)
				(pin output line
					(at 25.4 -43.18 180)
					(length 2.54)
					(name "PG4")
					(number "23")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "24")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "SYNC")
					(number "25")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{A}")
					(number "26")
				)
				(pin output line
					(at 25.4 -12.7 180)
					(length 2.54)
					(name "PG1")
					(number "27")
				)
				(pin passive line
					(at 25.4 -10.16 180)
					(length 2.54)
					(name "OUTS1")
					(number "28")
				)
				(pin power_in line
					(at 0 -50.8 0)
					(length 2.54)
					(name "EP")
					(number "29")
				)
			)
			(embedded_fonts no)
		)
)
