(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MAX20076ATCB_V+"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 31.75 -1.27 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MAX20076ATCB_V+"
				(at 31.75 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MAX20076ATCB_V+"
				(at 31.75 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/en/products/max20076.html"
				(at 31.75 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "DC-DC Switching Synchronous Step-Down Regulator, 3.5-36V in, 3.3V/1.2A out, 2.1MHz, TDFN-EP, 12Pin"
				(at 31.75 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MAX20076ATCB/V+"
				(at 31.75 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Analog Devices"
				(at 31.75 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 31.75 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 31.75 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, SWITCHING, VOLTAGE, REGULATOR, DC-DC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MAX20076ATCB_V+_1_1"
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SPS")
					(number "1")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "EN")
					(number "2")
				)
				(pin passive line
					(at 20.32 0 180)
					(length 2.54)
					(name "BST")
					(number "3")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "SUP")
					(number "4")
				)
				(pin power_out line
					(at 20.32 -7.62 180)
					(length 2.54)
					(name "LX")
					(number "5")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 2.54)
					(name "PGND")
					(number "6")
				)
				(pin power_in line
					(at 0 -22.86 0)
					(length 2.54)
					(name "AGND")
					(number "7")
				)
				(pin passive line
					(at 20.32 -12.7 180)
					(length 2.54)
					(name "FB")
					(number "8")
				)
				(pin passive line
					(at 20.32 -10.16 180)
					(length 2.54)
					(name "OUT")
					(number "9")
				)
				(pin passive line
					(at 20.32 -20.32 180)
					(length 2.54)
					(name "BIAS")
					(number "10")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "SYNC")
					(number "11")
				)
				(pin output line
					(at 0 -12.7 0)
					(length 2.54)
					(name "PGOOD")
					(number "12")
				)
				(pin power_in line
					(at 20.32 -22.86 180)
					(length 2.54)
					(name "EP")
					(number "13")
				)
			)
			(embedded_fonts no)
		)
)
