(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MIC5166YML-TR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 43.18 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MIC5166YML-TR"
				(at 43.18 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MIC5166YML-TR"
				(at 43.18 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/268/MIC5166_3A_High_Speed_Low_VIN_DDR_Terminator_DS200-1891162.pdf"
				(at 43.18 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Power distribution switch/load driver"
				(at 43.18 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MIC5166YML-TR"
				(at 43.18 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 43.18 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 43.18 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 43.18 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MIC5166YML-TR_1_1"
				(pin output line
					(at 27.94 -12.7 180)
					(length 2.54)
					(name "VREF")
					(number "1")
				)
				(pin power_in line
					(at 2.54 0 0)
					(length 2.54)
					(name "BIAS")
					(number "2")
				)
				(pin power_in line
					(at 2.54 -10.16 0)
					(length 2.54)
					(name "AGND")
					(number "3")
				)
				(pin input line
					(at 27.94 0 180)
					(length 2.54)
					(name "VDDQ")
					(number "4")
				)
				(pin output line
					(at 27.94 -10.16 180)
					(length 2.54)
					(name "PG")
					(number "5")
				)
				(pin input line
					(at 27.94 -5.08 180)
					(length 2.54)
					(name "SNS")
					(number "6")
				)
				(pin input line
					(at 2.54 -5.08 0)
					(length 2.54)
					(name "EN")
					(number "7")
				)
				(pin power_in line
					(at 2.54 -7.62 0)
					(length 2.54)
					(name "PGND")
					(number "8")
				)
				(pin power_out line
					(at 27.94 -2.54 180)
					(length 2.54)
					(name "VTT")
					(number "9")
				)
				(pin power_in line
					(at 2.54 -2.54 0)
					(length 2.54)
					(name "VIN")
					(number "10")
				)
				(pin power_in line
					(at 2.54 -12.7 0)
					(length 2.54)
					(name "EP")
					(number "11")
				)
			)
			(embedded_fonts no)
		)
)
