(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MIMXRT1187CVM8C"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 55.88 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MIMXRT1187CVM8C"
				(at 55.88 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MIMXRT1187CVM8C"
				(at 55.88 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/IMXRT1180RM.pdf"
				(at 55.88 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "i.MX RT1180: Crossover MCU with TSN Switch and EdgeLock -0.3 1.98 V,-55 150 C"
				(at 55.88 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MIMXRT1187CVM8C"
				(at 55.88 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "NXP"
				(at 55.88 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 55.88 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 55.88 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT, BGA, MICROCONTROLLER, ARM, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MIMXRT1187CVM8C_1_1"
				(pin passive line
					(at 41.91 -17.78 180)
					(length 5.08)
					(name "DAC_OUT")
					(number "J12")
				)
				(pin passive line
					(at 41.91 -2.54 180)
					(length 5.08)
					(name "WAKEUP")
					(number "T8")
				)
				(pin passive line
					(at 41.91 -10.16 180)
					(length 5.08)
					(name "PMIC_STBY_REQ")
					(number "T9")
				)
				(pin input line
					(at 41.91 -5.08 180)
					(length 5.08)
					(name "POR_B")
					(number "T10")
				)
				(pin input line
					(at 41.91 -22.86 180)
					(length 5.08)
					(name "TEST_MODE")
					(number "T11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "RTC_XTALI")
					(number "T13")
				)
				(pin no_connect line
					(at 0 -22.86 0)
					(length 5.08)
					(name "CLK1_N")
					(number "T15")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "XTALO")
					(number "T16")
				)
				(pin passive line
					(at 41.91 -12.7 180)
					(length 5.08)
					(name "PMIC_ON_REQ")
					(number "U9")
				)
				(pin input line
					(at 41.91 0 180)
					(length 5.08)
					(name "ONOFF")
					(number "U10")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "RTC_XTALO")
					(number "U13")
				)
				(pin no_connect line
					(at 0 -20.32 0)
					(length 5.08)
					(name "CLK1_P")
					(number "U15")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "XTALI")
					(number "U16")
				)
			)
			(symbol "MIMXRT1187CVM8C_2_1"
				(pin power_in line
					(at 0 -40.64 0)
					(length 5.08)
					(name "VDD_USB_1P8")
					(number "B17")
				)
				(pin power_in line
					(at 0 -38.1 0)
					(length 5.08)
					(name "VDD_USB_3P3")
					(number "G12")
				)
				(pin passive line
					(at 41.91 -20.32 180)
					(length 5.08)
					(name "ADC_VREFH")
					(number "H16")
				)
				(pin power_in line
					(at 41.91 -5.08 180)
					(length 5.08)
					(name "VDDA_ADC_1P8")
					(number "J13")
				)
				(pin power_in line
					(at 41.91 0 180)
					(length 5.08)
					(name "VDDA_ADC_3P3")
					(number "J14")
				)
				(pin power_in line
					(at 41.91 -10.16 180)
					(length 5.08)
					(name "VDDA_1P8_IN")
					(number "M12")
				)
				(pin passive line
					(at 41.91 -15.24 180)
					(length 5.08)
					(name "VDDA_1P0")
					(number "N11")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "VDD_AON_DIG")
					(number "P11")
				)
				(pin power_out line
					(at 0 -2.54 0)
					(length 5.08)
					(name "VDD_AON_ANA")
					(number "P12")
				)
				(pin power_out line
					(at 0 -12.7 0)
					(length 5.08)
					(name "VDD_BBSM_ANA")
					(number "R12")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 5.08)
					(name "VDD_BBSM_IN")
					(number "U12")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VDD_AON_IN")
					(number "U14")
				)
				(pin power_in line
					(at 0 -30.48 0)
					(length 5.08)
					(name "VDD_SOC")
					(number "[H8,H9,H10,J8,J9,J10,K10]")
				)
			)
			(symbol "MIMXRT1187CVM8C_3_1"
				(pin power_in line
					(at 0 -15.24 0)
					(length 5.08)
					(name "VSS")
					(number "[A1,A17,C11,C14,D4,D7,D8,D12,F11,F12]")
				)
				(pin power_in line
					(at 0 -29.21 0)
					(length 5.08)
					(name "VSS")
					(number "[F13,G4,G7,G8,G9,G10,G11]")
				)
				(pin power_in line
					(at 41.91 -15.24 180)
					(length 5.08)
					(name "VSS")
					(number "[G14,H7,H11,J7,J11,K11,L4,L10,L11,L14]")
				)
				(pin power_in line
					(at 41.91 -29.21 180)
					(length 5.08)
					(name "VSS")
					(number "[P3,P4,P7,P14,T12,U1,U17]")
				)
			)
			(symbol "MIMXRT1187CVM8C_4_1"
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(name "DCDC_PSWITCH")
					(number "L5")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(name "DCDC_MODE")
					(number "L6")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 5.08)
					(name "DCDC_IN_Q")
					(number "L7")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 5.08)
					(name "DCDC_SENSE")
					(number "L8")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(name "DCDC_1P8")
					(number "M4")
				)
				(pin power_in line
					(at 41.91 -26.67 180)
					(length 5.08)
					(name "DCDC_GND")
					(number "[K6,K7,K8,K9]")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "DCDC_IN")
					(number "[M5,M6,M7,M8]")
				)
				(pin power_out line
					(at 41.91 -2.54 180)
					(length 5.08)
					(name "DCDC_LP")
					(number "[T1,T2,T3,U2,U3]")
				)
			)
			(symbol "MIMXRT1187CVM8C_5_1"
				(pin bidirectional line
					(at 41.91 -10.16 180)
					(length 5.08)
					(name "USB2_DN")
					(number "C16")
				)
				(pin bidirectional line
					(at 41.91 -7.62 180)
					(length 5.08)
					(name "USB2_DP")
					(number "C17")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "USB2_VBUS")
					(number "D16")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "USB1_VBUS")
					(number "D17")
				)
				(pin bidirectional line
					(at 41.91 -2.54 180)
					(length 5.08)
					(name "USB1_DN")
					(number "E16")
				)
				(pin bidirectional line
					(at 41.91 0 180)
					(length 5.08)
					(name "USB1_DP")
					(number "E17")
				)
			)
			(symbol "MIMXRT1187CVM8C_6_1"
				(pin passive line
					(at 41.91 -5.08 180)
					(length 5.08)
					(name "GPIO_BBSM_02")
					(number "L9")
				)
				(pin passive line
					(at 41.91 -15.24 180)
					(length 5.08)
					(name "GPIO_BBSM_06")
					(number "M9")
				)
				(pin passive line
					(at 41.91 -7.62 180)
					(length 5.08)
					(name "GPIO_BBSM_03")
					(number "M10")
				)
				(pin passive line
					(at 41.91 -20.32 180)
					(length 5.08)
					(name "GPIO_BBSM_08")
					(number "N9")
				)
				(pin passive line
					(at 41.91 -10.16 180)
					(length 5.08)
					(name "GPIO_BBSM_04")
					(number "N10")
				)
				(pin passive line
					(at 41.91 -12.7 180)
					(length 5.08)
					(name "GPIO_BBSM_05")
					(number "P9")
				)
				(pin passive line
					(at 41.91 -2.54 180)
					(length 5.08)
					(name "GPIO_BBSM_01")
					(number "P10")
				)
				(pin passive line
					(at 41.91 -17.78 180)
					(length 5.08)
					(name "GPIO_BBSM_07")
					(number "R9")
				)
				(pin passive line
					(at 41.91 0 180)
					(length 5.08)
					(name "GPIO_BBSM_00")
					(number "R10")
				)
				(pin passive line
					(at 41.91 -22.86 180)
					(length 5.08)
					(name "GPIO_BBSM_09")
					(number "R11")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "NVCC_BBSM")
					(number "U11")
				)
			)
			(symbol "MIMXRT1187CVM8C_7_1"
				(pin bidirectional line
					(at 41.91 -33.02 180)
					(length 5.08)
					(name "GPIO_AON_13")
					(number "A2")
				)
				(pin bidirectional line
					(at 41.91 -30.48 180)
					(length 5.08)
					(name "GPIO_AON_12")
					(number "A3")
				)
				(pin bidirectional line
					(at 41.91 -27.94 180)
					(length 5.08)
					(name "GPIO_AON_11")
					(number "A4")
				)
				(pin bidirectional line
					(at 41.91 -22.86 180)
					(length 5.08)
					(name "GPIO_AON_09")
					(number "A5")
				)
				(pin bidirectional line
					(at 41.91 -20.32 180)
					(length 5.08)
					(name "GPIO_AON_08")
					(number "B1")
				)
				(pin bidirectional line
					(at 41.91 -35.56 180)
					(length 5.08)
					(name "GPIO_AON_14")
					(number "B2")
				)
				(pin bidirectional line
					(at 41.91 -38.1 180)
					(length 5.08)
					(name "GPIO_AON_15")
					(number "B3")
				)
				(pin bidirectional line
					(at 41.91 -10.16 180)
					(length 5.08)
					(name "GPIO_AON_04")
					(number "B4")
				)
				(pin bidirectional line
					(at 41.91 -25.4 180)
					(length 5.08)
					(name "GPIO_AON_10")
					(number "B5")
				)
				(pin bidirectional line
					(at 41.91 -5.08 180)
					(length 5.08)
					(name "GPIO_AON_02")
					(number "B6")
				)
				(pin bidirectional line
					(at 41.91 -2.54 180)
					(length 5.08)
					(name "GPIO_AON_01")
					(number "B7")
				)
				(pin bidirectional line
					(at 41.91 -60.96 180)
					(length 5.08)
					(name "GPIO_AON_24")
					(number "C1")
				)
				(pin bidirectional line
					(at 41.91 -58.42 180)
					(length 5.08)
					(name "GPIO_AON_23")
					(number "C2")
				)
				(pin bidirectional line
					(at 41.91 -55.88 180)
					(length 5.08)
					(name "GPIO_AON_22")
					(number "C3")
				)
				(pin bidirectional line
					(at 41.91 -66.04 180)
					(length 5.08)
					(name "GPIO_AON_26")
					(number "C4")
				)
				(pin bidirectional line
					(at 41.91 -40.64 180)
					(length 5.08)
					(name "GPIO_AON_16")
					(number "C5")
				)
				(pin bidirectional line
					(at 41.91 -17.78 180)
					(length 5.08)
					(name "GPIO_AON_07")
					(number "C6")
				)
				(pin bidirectional line
					(at 41.91 -12.7 180)
					(length 5.08)
					(name "GPIO_AON_05")
					(number "C7")
				)
				(pin bidirectional line
					(at 41.91 -7.62 180)
					(length 5.08)
					(name "GPIO_AON_03")
					(number "C8")
				)
				(pin bidirectional line
					(at 41.91 -63.5 180)
					(length 5.08)
					(name "GPIO_AON_25")
					(number "D2")
				)
				(pin bidirectional line
					(at 41.91 -68.58 180)
					(length 5.08)
					(name "GPIO_AON_27")
					(number "D3")
				)
				(pin bidirectional line
					(at 41.91 -48.26 180)
					(length 5.08)
					(name "GPIO_AON_19")
					(number "D5")
				)
				(pin bidirectional line
					(at 41.91 -43.18 180)
					(length 5.08)
					(name "GPIO_AON_17")
					(number "D6")
				)
				(pin bidirectional line
					(at 41.91 -50.8 180)
					(length 5.08)
					(name "GPIO_AON_20")
					(number "E5")
				)
				(pin bidirectional line
					(at 41.91 -45.72 180)
					(length 5.08)
					(name "GPIO_AON_18")
					(number "E6")
				)
				(pin bidirectional line
					(at 41.91 -15.24 180)
					(length 5.08)
					(name "GPIO_AON_06")
					(number "E7")
				)
				(pin bidirectional line
					(at 41.91 -53.34 180)
					(length 5.08)
					(name "GPIO_AON_21")
					(number "F6")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "NVCC_AON")
					(number "F7")
				)
				(pin bidirectional line
					(at 41.91 0 180)
					(length 5.08)
					(name "GPIO_AON_00")
					(number "F8")
				)
			)
			(symbol "MIMXRT1187CVM8C_8_1"
				(pin bidirectional line
					(at 41.91 -88.9 180)
					(length 5.08)
					(name "GPIO_AD_35")
					(number "H17")
				)
				(pin bidirectional line
					(at 41.91 -86.36 180)
					(length 5.08)
					(name "GPIO_AD_34")
					(number "J15")
				)
				(pin bidirectional line
					(at 41.91 -83.82 180)
					(length 5.08)
					(name "GPIO_AD_33")
					(number "J16")
				)
				(pin bidirectional line
					(at 41.91 -81.28 180)
					(length 5.08)
					(name "GPIO_AD_32")
					(number "J17")
				)
				(pin bidirectional line
					(at 41.91 -55.88 180)
					(length 5.08)
					(name "GPIO_AD_22")
					(number "K12")
				)
				(pin bidirectional line
					(at 41.91 -50.8 180)
					(length 5.08)
					(name "GPIO_AD_20")
					(number "K13")
				)
				(pin bidirectional line
					(at 41.91 -58.42 180)
					(length 5.08)
					(name "GPIO_AD_23")
					(number "K14")
				)
				(pin bidirectional line
					(at 41.91 -53.34 180)
					(length 5.08)
					(name "GPIO_AD_21")
					(number "K15")
				)
				(pin bidirectional line
					(at 41.91 -45.72 180)
					(length 5.08)
					(name "GPIO_AD_18")
					(number "K16")
				)
				(pin bidirectional line
					(at 41.91 -78.74 180)
					(length 5.08)
					(name "GPIO_AD_31")
					(number "K17")
				)
				(pin bidirectional line
					(at 41.91 -48.26 180)
					(length 5.08)
					(name "GPIO_AD_19")
					(number "L13")
				)
				(pin bidirectional line
					(at 41.91 -73.66 180)
					(length 5.08)
					(name "GPIO_AD_29")
					(number "L15")
				)
				(pin bidirectional line
					(at 41.91 -71.12 180)
					(length 5.08)
					(name "GPIO_AD_28")
					(number "L16")
				)
				(pin bidirectional line
					(at 41.91 -76.2 180)
					(length 5.08)
					(name "GPIO_AD_30")
					(number "L17")
				)
				(pin bidirectional line
					(at 41.91 -60.96 180)
					(length 5.08)
					(name "GPIO_AD_24")
					(number "M13")
				)
				(pin bidirectional line
					(at 41.91 -66.04 180)
					(length 5.08)
					(name "GPIO_AD_26")
					(number "M14")
				)
				(pin bidirectional line
					(at 41.91 -63.5 180)
					(length 5.08)
					(name "GPIO_AD_25")
					(number "M15")
				)
				(pin bidirectional line
					(at 41.91 -68.58 180)
					(length 5.08)
					(name "GPIO_AD_27")
					(number "M16")
				)
				(pin bidirectional line
					(at 41.91 -43.18 180)
					(length 5.08)
					(name "GPIO_AD_17")
					(number "M17")
				)
				(pin bidirectional line
					(at 41.91 0 180)
					(length 5.08)
					(name "GPIO_AD_00")
					(number "N12")
				)
				(pin bidirectional line
					(at 41.91 -15.24 180)
					(length 5.08)
					(name "GPIO_AD_06")
					(number "N13")
				)
				(pin bidirectional line
					(at 41.91 -35.56 180)
					(length 5.08)
					(name "GPIO_AD_14")
					(number "N14")
				)
				(pin bidirectional line
					(at 41.91 -33.02 180)
					(length 5.08)
					(name "GPIO_AD_13")
					(number "N15")
				)
				(pin bidirectional line
					(at 41.91 -38.1 180)
					(length 5.08)
					(name "GPIO_AD_15")
					(number "N16")
				)
				(pin bidirectional line
					(at 41.91 -40.64 180)
					(length 5.08)
					(name "GPIO_AD_16")
					(number "N17")
				)
				(pin bidirectional line
					(at 41.91 -12.7 180)
					(length 5.08)
					(name "GPIO_AD_05")
					(number "P13")
				)
				(pin bidirectional line
					(at 41.91 -10.16 180)
					(length 5.08)
					(name "GPIO_AD_04")
					(number "P15")
				)
				(pin bidirectional line
					(at 41.91 -27.94 180)
					(length 5.08)
					(name "GPIO_AD_11")
					(number "P16")
				)
				(pin bidirectional line
					(at 41.91 -30.48 180)
					(length 5.08)
					(name "GPIO_AD_12")
					(number "P17")
				)
				(pin bidirectional line
					(at 41.91 -5.08 180)
					(length 5.08)
					(name "GPIO_AD_02")
					(number "R13")
				)
				(pin bidirectional line
					(at 41.91 -2.54 180)
					(length 5.08)
					(name "GPIO_AD_01")
					(number "R14")
				)
				(pin bidirectional line
					(at 41.91 -7.62 180)
					(length 5.08)
					(name "GPIO_AD_03")
					(number "R15")
				)
				(pin bidirectional line
					(at 41.91 -22.86 180)
					(length 5.08)
					(name "GPIO_AD_09")
					(number "R16")
				)
				(pin bidirectional line
					(at 41.91 -25.4 180)
					(length 5.08)
					(name "GPIO_AD_10")
					(number "R17")
				)
				(pin bidirectional line
					(at 41.91 -20.32 180)
					(length 5.08)
					(name "GPIO_AD_08")
					(number "T14")
				)
				(pin bidirectional line
					(at 41.91 -17.78 180)
					(length 5.08)
					(name "GPIO_AD_07")
					(number "T17")
				)
				(pin power_in line
					(at 0 -1.27 0)
					(length 5.08)
					(name "NVCC_GPIO_AD")
					(number "[L12,M11]")
				)
			)
			(symbol "MIMXRT1187CVM8C_9_1"
				(pin bidirectional line
					(at 41.91 -30.48 180)
					(length 5.08)
					(name "GPIO_B1_12")
					(number "A11")
				)
				(pin bidirectional line
					(at 41.91 -27.94 180)
					(length 5.08)
					(name "GPIO_B1_11")
					(number "A12")
				)
				(pin bidirectional line
					(at 41.91 -25.4 180)
					(length 5.08)
					(name "GPIO_B1_10")
					(number "A13")
				)
				(pin bidirectional line
					(at 41.91 -7.62 180)
					(length 5.08)
					(name "GPIO_B1_03")
					(number "A14")
				)
				(pin bidirectional line
					(at 41.91 -22.86 180)
					(length 5.08)
					(name "GPIO_B1_09")
					(number "A15")
				)
				(pin bidirectional line
					(at 41.91 -15.24 180)
					(length 5.08)
					(name "GPIO_B1_06")
					(number "B10")
				)
				(pin bidirectional line
					(at 41.91 -33.02 180)
					(length 5.08)
					(name "GPIO_B1_13")
					(number "B11")
				)
				(pin bidirectional line
					(at 41.91 -12.7 180)
					(length 5.08)
					(name "GPIO_B1_05")
					(number "B12")
				)
				(pin bidirectional line
					(at 41.91 -10.16 180)
					(length 5.08)
					(name "GPIO_B1_04")
					(number "B13")
				)
				(pin bidirectional line
					(at 41.91 -20.32 180)
					(length 5.08)
					(name "GPIO_B1_08")
					(number "B14")
				)
				(pin bidirectional line
					(at 41.91 -2.54 180)
					(length 5.08)
					(name "GPIO_B1_01")
					(number "C12")
				)
				(pin bidirectional line
					(at 41.91 -17.78 180)
					(length 5.08)
					(name "GPIO_B1_07")
					(number "D13")
				)
				(pin bidirectional line
					(at 41.91 -5.08 180)
					(length 5.08)
					(name "GPIO_B1_02")
					(number "E12")
				)
				(pin bidirectional line
					(at 41.91 0 180)
					(length 5.08)
					(name "GPIO_B1_00")
					(number "E13")
				)
				(pin power_in line
					(at 0 -1.27 0)
					(length 5.08)
					(name "NVCC_GPIO1")
					(number "[D11,E11]")
				)
			)
			(symbol "MIMXRT1187CVM8C_10_1"
				(pin bidirectional line
					(at 41.91 -17.78 180)
					(length 5.08)
					(name "GPIO_B2_07")
					(number "A6")
				)
				(pin bidirectional line
					(at 41.91 -20.32 180)
					(length 5.08)
					(name "GPIO_B2_08")
					(number "A7")
				)
				(pin bidirectional line
					(at 41.91 -30.48 180)
					(length 5.08)
					(name "GPIO_B2_12")
					(number "A8")
				)
				(pin bidirectional line
					(at 41.91 -12.7 180)
					(length 5.08)
					(name "GPIO_B2_05")
					(number "A9")
				)
				(pin bidirectional line
					(at 41.91 -25.4 180)
					(length 5.08)
					(name "GPIO_B2_10")
					(number "A10")
				)
				(pin bidirectional line
					(at 41.91 -33.02 180)
					(length 5.08)
					(name "GPIO_B2_13")
					(number "B8")
				)
				(pin bidirectional line
					(at 41.91 -27.94 180)
					(length 5.08)
					(name "GPIO_B2_11")
					(number "B9")
				)
				(pin bidirectional line
					(at 41.91 -10.16 180)
					(length 5.08)
					(name "GPIO_B2_04")
					(number "C9")
				)
				(pin bidirectional line
					(at 41.91 -5.08 180)
					(length 5.08)
					(name "GPIO_B2_02")
					(number "C10")
				)
				(pin bidirectional line
					(at 41.91 -7.62 180)
					(length 5.08)
					(name "GPIO_B2_03")
					(number "D9")
				)
				(pin bidirectional line
					(at 41.91 -22.86 180)
					(length 5.08)
					(name "GPIO_B2_09")
					(number "D10")
				)
				(pin bidirectional line
					(at 41.91 -15.24 180)
					(length 5.08)
					(name "GPIO_B2_06")
					(number "E8")
				)
				(pin bidirectional line
					(at 41.91 0 180)
					(length 5.08)
					(name "GPIO_B2_00")
					(number "E9")
				)
				(pin bidirectional line
					(at 41.91 -2.54 180)
					(length 5.08)
					(name "GPIO_B2_01")
					(number "E10")
				)
				(pin power_in line
					(at 0 -1.27 0)
					(length 5.08)
					(name "NVCC_GPIO2")
					(number "[F9,F10]")
				)
			)
			(symbol "MIMXRT1187CVM8C_11_1"
				(pin bidirectional line
					(at 41.91 -12.7 180)
					(length 5.08)
					(name "GPIO_SD_B1_05")
					(number "A16")
				)
				(pin bidirectional line
					(at 41.91 -10.16 180)
					(length 5.08)
					(name "GPIO_SD_B1_04")
					(number "B15")
				)
				(pin bidirectional line
					(at 41.91 0 180)
					(length 5.08)
					(name "GPIO_SD_B1_00")
					(number "B16")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "NVCC_SD1")
					(number "C13")
				)
				(pin bidirectional line
					(at 41.91 -7.62 180)
					(length 5.08)
					(name "GPIO_SD_B1_03")
					(number "C15")
				)
				(pin bidirectional line
					(at 41.91 -5.08 180)
					(length 5.08)
					(name "GPIO_SD_B1_02")
					(number "D14")
				)
				(pin bidirectional line
					(at 41.91 -2.54 180)
					(length 5.08)
					(name "GPIO_SD_B1_01")
					(number "D15")
				)
			)
			(symbol "MIMXRT1187CVM8C_12_1"
				(pin bidirectional line
					(at 41.91 -17.78 180)
					(length 5.08)
					(name "GPIO_SD_B2_07")
					(number "E14")
				)
				(pin bidirectional line
					(at 41.91 -12.7 180)
					(length 5.08)
					(name "GPIO_SD_B2_05")
					(number "E15")
				)
				(pin bidirectional line
					(at 41.91 -20.32 180)
					(length 5.08)
					(name "GPIO_SD_B2_08")
					(number "F14")
				)
				(pin bidirectional line
					(at 41.91 -15.24 180)
					(length 5.08)
					(name "GPIO_SD_B2_06")
					(number "F15")
				)
				(pin bidirectional line
					(at 41.91 -22.86 180)
					(length 5.08)
					(name "GPIO_SD_B2_09")
					(number "F16")
				)
				(pin bidirectional line
					(at 41.91 -27.94 180)
					(length 5.08)
					(name "GPIO_SD_B2_11")
					(number "F17")
				)
				(pin bidirectional line
					(at 41.91 -7.62 180)
					(length 5.08)
					(name "GPIO_SD_B2_03")
					(number "G13")
				)
				(pin bidirectional line
					(at 41.91 -10.16 180)
					(length 5.08)
					(name "GPIO_SD_B2_04")
					(number "G15")
				)
				(pin bidirectional line
					(at 41.91 -25.4 180)
					(length 5.08)
					(name "GPIO_SD_B2_10")
					(number "G16")
				)
				(pin bidirectional line
					(at 41.91 -5.08 180)
					(length 5.08)
					(name "GPIO_SD_B2_02")
					(number "G17")
				)
				(pin bidirectional line
					(at 41.91 -2.54 180)
					(length 5.08)
					(name "GPIO_SD_B2_01")
					(number "H14")
				)
				(pin bidirectional line
					(at 41.91 0 180)
					(length 5.08)
					(name "GPIO_SD_B2_00")
					(number "H15")
				)
				(pin power_in line
					(at 0 -1.27 0)
					(length 5.08)
					(name "NVCC_SD2")
					(number "[H12,H13]")
				)
			)
			(symbol "MIMXRT1187CVM8C_13_1"
				(pin bidirectional line
					(at 41.91 -45.72 180)
					(length 5.08)
					(name "GPIO_EMC_B1_18")
					(number "D1")
				)
				(pin bidirectional line
					(at 41.91 -22.86 180)
					(length 5.08)
					(name "GPIO_EMC_B1_09")
					(number "E1")
				)
				(pin bidirectional line
					(at 41.91 -43.18 180)
					(length 5.08)
					(name "GPIO_EMC_B1_17")
					(number "E2")
				)
				(pin bidirectional line
					(at 41.91 -25.4 180)
					(length 5.08)
					(name "GPIO_EMC_B1_10")
					(number "E3")
				)
				(pin bidirectional line
					(at 41.91 -73.66 180)
					(length 5.08)
					(name "GPIO_EMC_B1_29")
					(number "E4")
				)
				(pin bidirectional line
					(at 41.91 -58.42 180)
					(length 5.08)
					(name "GPIO_EMC_B1_23")
					(number "F1")
				)
				(pin bidirectional line
					(at 41.91 -27.94 180)
					(length 5.08)
					(name "GPIO_EMC_B1_11")
					(number "F2")
				)
				(pin bidirectional line
					(at 41.91 -33.02 180)
					(length 5.08)
					(name "GPIO_EMC_B1_13")
					(number "F3")
				)
				(pin bidirectional line
					(at 41.91 -48.26 180)
					(length 5.08)
					(name "GPIO_EMC_B1_19")
					(number "F4")
				)
				(pin bidirectional line
					(at 41.91 -71.12 180)
					(length 5.08)
					(name "GPIO_EMC_B1_28")
					(number "F5")
				)
				(pin bidirectional line
					(at 41.91 -50.8 180)
					(length 5.08)
					(name "GPIO_EMC_B1_20")
					(number "G1")
				)
				(pin bidirectional line
					(at 41.91 -38.1 180)
					(length 5.08)
					(name "GPIO_EMC_B1_15")
					(number "G2")
				)
				(pin bidirectional line
					(at 41.91 -7.62 180)
					(length 5.08)
					(name "GPIO_EMC_B1_03")
					(number "G3")
				)
				(pin bidirectional line
					(at 41.91 -35.56 180)
					(length 5.08)
					(name "GPIO_EMC_B1_14")
					(number "G5")
				)
				(pin bidirectional line
					(at 41.91 -30.48 180)
					(length 5.08)
					(name "GPIO_EMC_B1_12")
					(number "G6")
				)
				(pin bidirectional line
					(at 41.91 -40.64 180)
					(length 5.08)
					(name "GPIO_EMC_B1_16")
					(number "H1")
				)
				(pin bidirectional line
					(at 41.91 -76.2 180)
					(length 5.08)
					(name "GPIO_EMC_B1_30")
					(number "H2")
				)
				(pin bidirectional line
					(at 41.91 0 180)
					(length 5.08)
					(name "GPIO_EMC_B1_00")
					(number "H3")
				)
				(pin bidirectional line
					(at 41.91 -2.54 180)
					(length 5.08)
					(name "GPIO_EMC_B1_01")
					(number "H4")
				)
				(pin bidirectional line
					(at 41.91 -20.32 180)
					(length 5.08)
					(name "GPIO_EMC_B1_08")
					(number "H5")
				)
				(pin bidirectional line
					(at 41.91 -12.7 180)
					(length 5.08)
					(name "GPIO_EMC_B1_05")
					(number "H6")
				)
				(pin bidirectional line
					(at 41.91 -81.28 180)
					(length 5.08)
					(name "GPIO_EMC_B1_32")
					(number "J1")
				)
				(pin bidirectional line
					(at 41.91 -78.74 180)
					(length 5.08)
					(name "GPIO_EMC_B1_31")
					(number "J2")
				)
				(pin bidirectional line
					(at 41.91 -68.58 180)
					(length 5.08)
					(name "GPIO_EMC_B1_27")
					(number "J3")
				)
				(pin bidirectional line
					(at 41.91 -10.16 180)
					(length 5.08)
					(name "GPIO_EMC_B1_04")
					(number "J4")
				)
				(pin bidirectional line
					(at 41.91 -83.82 180)
					(length 5.08)
					(name "GPIO_EMC_B1_33")
					(number "K1")
				)
				(pin bidirectional line
					(at 41.91 -5.08 180)
					(length 5.08)
					(name "GPIO_EMC_B1_02")
					(number "K2")
				)
				(pin bidirectional line
					(at 41.91 -15.24 180)
					(length 5.08)
					(name "GPIO_EMC_B1_06")
					(number "K3")
				)
				(pin bidirectional line
					(at 41.91 -53.34 180)
					(length 5.08)
					(name "GPIO_EMC_B1_21")
					(number "K4")
				)
				(pin bidirectional line
					(at 41.91 -88.9 180)
					(length 5.08)
					(name "GPIO_EMC_B1_35")
					(number "L1")
				)
				(pin bidirectional line
					(at 41.91 -86.36 180)
					(length 5.08)
					(name "GPIO_EMC_B1_34")
					(number "L2")
				)
				(pin bidirectional line
					(at 41.91 -55.88 180)
					(length 5.08)
					(name "GPIO_EMC_B1_22")
					(number "L3")
				)
				(pin bidirectional line
					(at 41.91 -91.44 180)
					(length 5.08)
					(name "GPIO_EMC_B1_36")
					(number "M1")
				)
				(pin bidirectional line
					(at 41.91 -96.52 180)
					(length 5.08)
					(name "GPIO_EMC_B1_38")
					(number "M2")
				)
				(pin bidirectional line
					(at 41.91 -17.78 180)
					(length 5.08)
					(name "GPIO_EMC_B1_07")
					(number "M3")
				)
				(pin bidirectional line
					(at 41.91 -93.98 180)
					(length 5.08)
					(name "GPIO_EMC_B1_37")
					(number "N1")
				)
				(pin bidirectional line
					(at 41.91 -101.6 180)
					(length 5.08)
					(name "GPIO_EMC_B1_40")
					(number "N2")
				)
				(pin bidirectional line
					(at 41.91 -63.5 180)
					(length 5.08)
					(name "GPIO_EMC_B1_25")
					(number "N3")
				)
				(pin bidirectional line
					(at 41.91 -66.04 180)
					(length 5.08)
					(name "GPIO_EMC_B1_26")
					(number "N4")
				)
				(pin bidirectional line
					(at 41.91 -99.06 180)
					(length 5.08)
					(name "GPIO_EMC_B1_39")
					(number "P1")
				)
				(pin bidirectional line
					(at 41.91 -60.96 180)
					(length 5.08)
					(name "GPIO_EMC_B1_24")
					(number "P2")
				)
				(pin bidirectional line
					(at 41.91 -104.14 180)
					(length 5.08)
					(name "GPIO_EMC_B1_41")
					(number "R1")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 5.08)
					(name "NVCC_EMC1")
					(number "[J5,J6,K5]")
				)
			)
			(symbol "MIMXRT1187CVM8C_14_1"
				(pin bidirectional line
					(at 41.91 0 180)
					(length 5.08)
					(name "GPIO_EMC_B2_00")
					(number "N5")
				)
				(pin bidirectional line
					(at 41.91 -35.56 180)
					(length 5.08)
					(name "GPIO_EMC_B2_14")
					(number "N8")
				)
				(pin bidirectional line
					(at 41.91 -5.08 180)
					(length 5.08)
					(name "GPIO_EMC_B2_02")
					(number "P5")
				)
				(pin bidirectional line
					(at 41.91 -27.94 180)
					(length 5.08)
					(name "GPIO_EMC_B2_11")
					(number "P6")
				)
				(pin bidirectional line
					(at 41.91 -45.72 180)
					(length 5.08)
					(name "GPIO_EMC_B2_18")
					(number "P8")
				)
				(pin bidirectional line
					(at 41.91 -2.54 180)
					(length 5.08)
					(name "GPIO_EMC_B2_01")
					(number "R2")
				)
				(pin bidirectional line
					(at 41.91 -10.16 180)
					(length 5.08)
					(name "GPIO_EMC_B2_04")
					(number "R3")
				)
				(pin bidirectional line
					(at 41.91 -38.1 180)
					(length 5.08)
					(name "GPIO_EMC_B2_15")
					(number "R4")
				)
				(pin bidirectional line
					(at 41.91 -30.48 180)
					(length 5.08)
					(name "GPIO_EMC_B2_12")
					(number "R5")
				)
				(pin bidirectional line
					(at 41.91 -33.02 180)
					(length 5.08)
					(name "GPIO_EMC_B2_13")
					(number "R6")
				)
				(pin bidirectional line
					(at 41.91 -40.64 180)
					(length 5.08)
					(name "GPIO_EMC_B2_16")
					(number "R7")
				)
				(pin bidirectional line
					(at 41.91 -50.8 180)
					(length 5.08)
					(name "GPIO_EMC_B2_20")
					(number "R8")
				)
				(pin bidirectional line
					(at 41.91 -12.7 180)
					(length 5.08)
					(name "GPIO_EMC_B2_05")
					(number "T4")
				)
				(pin bidirectional line
					(at 41.91 -7.62 180)
					(length 5.08)
					(name "GPIO_EMC_B2_03")
					(number "T5")
				)
				(pin bidirectional line
					(at 41.91 -15.24 180)
					(length 5.08)
					(name "GPIO_EMC_B2_06")
					(number "T6")
				)
				(pin bidirectional line
					(at 41.91 -17.78 180)
					(length 5.08)
					(name "GPIO_EMC_B2_07")
					(number "T7")
				)
				(pin bidirectional line
					(at 41.91 -20.32 180)
					(length 5.08)
					(name "GPIO_EMC_B2_08")
					(number "U4")
				)
				(pin bidirectional line
					(at 41.91 -22.86 180)
					(length 5.08)
					(name "GPIO_EMC_B2_09")
					(number "U5")
				)
				(pin bidirectional line
					(at 41.91 -25.4 180)
					(length 5.08)
					(name "GPIO_EMC_B2_10")
					(number "U6")
				)
				(pin bidirectional line
					(at 41.91 -43.18 180)
					(length 5.08)
					(name "GPIO_EMC_B2_17")
					(number "U7")
				)
				(pin bidirectional line
					(at 41.91 -48.26 180)
					(length 5.08)
					(name "GPIO_EMC_B2_19")
					(number "U8")
				)
				(pin power_in line
					(at 0 -1.27 0)
					(length 5.08)
					(name "NVCC_EMC2")
					(number "[N6,N7]")
				)
			)
			(embedded_fonts no)
		)
)
