(footprint "QFN-26_3.5x4.5x1mm_P0.45mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -2.8 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-26_3.5x4.5x1mm_P0.45mm"
		(at 0 3.7 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -2.65 7.195 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -2.65 8.395 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -2.65 9.595 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.61 -1.855)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd roundrect
		(at -1.29 -1.905 90)
		(size 0.3 0.525)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0)
		(chamfer_ratio 0.5)
		(chamfer bottom_left)
	)
	(pad "1" smd rect
		(at -1.125 -2.23 90)
		(size 0.65 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.6 -1.405)
		(size 0.9 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.4 -0.955)
		(size 1.3 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.4 -0.505)
		(size 1.3 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -1.4 -0.005)
		(size 1.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -1.4 0.495)
		(size 1.3 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -1.4 0.945)
		(size 1.3 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -1.6 1.395)
		(size 0.9 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -1.54 1.845)
		(size 1.025 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -1.29 1.895 90)
		(size 0.3 0.525)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -1.125 2.145 90)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -0.675 2.095 90)
		(size 0.9 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -0.225 2.095 90)
		(size 0.9 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 0.225 2.095 90)
		(size 0.9 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 0.675 2.095 90)
		(size 0.9 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 1.125 2.145 90)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 1.29 1.895 90)
		(size 0.3 0.525)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 1.54 1.845)
		(size 1.025 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 1.6 1.395)
		(size 0.9 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 1.4 0.945)
		(size 1.3 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 1.4 0.495)
		(size 1.3 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 1.4 -0.005)
		(size 1.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 1.4 -0.505)
		(size 1.3 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 1.4 -0.955)
		(size 1.3 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 1.6 -1.405)
		(size 0.9 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 1.125 -2.155 90)
		(size 0.8 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 1.29 -1.905 90)
		(size 0.3 0.525)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 1.54 -1.855)
		(size 1.025 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 0.675 -2.105 90)
		(size 0.9 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 0.225 -2.105 90)
		(size 0.9 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at -0.225 -2.105 90)
		(size 0.9 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at -0.675 -2.105 90)
		(size 0.9 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_mp5424grm_0000_z.glb"
		(offset
			(xyz -25.615 -15.245 0.1)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
