(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MP5424GRM"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 41.91 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MP5424GRM"
				(at 41.91 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MP5424GRM"
				(at 41.91 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.monolithicpower.com/en/documentview/productdocument/index/version/2/document_type/Datasheet/lang/en/sku/MP5424GRM/document_id/10311/"
				(at 41.91 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "5V PMIC with Four 4.5A/2.5A/4.5A/2A Buck Converters, 3 LDOs, 1 Load Switch and Flexible System Settings via I2C and MTP"
				(at 41.91 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MP5424GRM-0000-Z"
				(at 41.91 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Monolithic Power Systems"
				(at 41.91 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 41.91 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 41.91 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, VOLTAGE, REGULATOR, SWITCHING, DC-DC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MP5424GRM_0_1")
			(symbol "MP5424GRM_1_1"
				(pin input line
					(at 25.4 -2.54 180)
					(length 2.54)
					(name "FB1")
					(number "1")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "PWRON")
					(number "2")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VIN1")
					(number "3")
				)
				(pin power_out line
					(at 25.4 0 180)
					(length 2.54)
					(name "SW1")
					(number "4")
				)
				(pin power_in line
					(at 0 -45.72 0)
					(length 2.54)
					(name "GND")
					(number "5")
				)
				(pin power_out line
					(at 25.4 -20.32 180)
					(length 2.54)
					(name "SW3")
					(number "6")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VIN3")
					(number "7")
				)
				(pin input line
					(at 25.4 -22.86 180)
					(length 2.54)
					(name "FB3")
					(number "8")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "RSTO")
					(number "9")
				)
				(pin input line
					(at 0 -36.83 0)
					(length 2.54)
					(name "SCL")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 2.54)
					(name "SDA")
					(number "11")
				)
				(pin power_out line
					(at 25.4 -35.56 180)
					(length 2.54)
					(name "OUT4")
					(number "12")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "VIN5")
					(number "13")
				)
				(pin power_out line
					(at 25.4 -40.64 180)
					(length 2.54)
					(name "OUT5")
					(number "14")
				)
				(pin input line
					(at 25.4 -30.48 180)
					(length 2.54)
					(name "FB4")
					(number "15")
				)
				(pin power_in line
					(at 0 -11.43 0)
					(length 2.54)
					(name "VIN4")
					(number "16")
				)
				(pin power_out line
					(at 25.4 -27.94 180)
					(length 2.54)
					(name "SW4")
					(number "17")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 2.54)
					(name "GND")
					(number "18")
				)
				(pin power_out line
					(at 25.4 -7.62 180)
					(length 2.54)
					(name "SW2")
					(number "19")
				)
				(pin power_in line
					(at 0 -3.81 0)
					(length 2.54)
					(name "VIN2")
					(number "20")
				)
				(pin input line
					(at 25.4 -10.16 180)
					(length 2.54)
					(name "FB2")
					(number "21")
				)
				(pin power_out line
					(at 25.4 -15.24 180)
					(length 2.54)
					(name "OUT2")
					(number "22")
				)
				(pin power_in line
					(at 0 -19.05 0)
					(length 2.54)
					(name "LSWI")
					(number "23")
				)
				(pin power_out line
					(at 25.4 -45.72 180)
					(length 2.54)
					(name "LSWO")
					(number "24")
				)
				(pin power_in line
					(at 0 -43.18 0)
					(length 2.54)
					(name "AGND")
					(number "25")
				)
				(pin input line
					(at 0 -24.13 0)
					(length 2.54)
					(name "AVIN")
					(number "26")
				)
			)
			(embedded_fonts no)
		)
)
