(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MP8869S"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 25.4 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MP8869S"
				(at 25.4 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MP8869S"
				(at 25.4 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/277/MP8869S-2946178.pdf"
				(at 25.4 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "DC-DC Switching Synchronous Buck Regulator, 2.85V-18V in, 600mV to 5.5V out, 12A, 500kHz, QFN-14"
				(at 25.4 -26.67 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MP8869SGL-P"
				(at 25.4 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Monolithic Power Systems"
				(at 25.4 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 25.4 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 25.4 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, VOLTAGE, REGULATOR, SWITCHING, DC-DC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "QFN-14_MP8869S_MNP"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MP8869S_1_1"
				(pin unspecified line
					(at 0 0 270)
					(length 2.54)
					(name "BST")
					(number "1")
				)
				(pin output line
					(at 10.16 -5.08 180)
					(length 2.54)
					(name "SW")
					(number "2")
				)
				(pin unspecified line
					(at -10.16 -25.4 0)
					(length 2.54)
					(name "SCL")
					(number "3")
				)
				(pin unspecified line
					(at -10.16 -22.86 0)
					(length 2.54)
					(name "SDA")
					(number "4")
				)
				(pin unspecified line
					(at -10.16 -10.16 0)
					(length 2.54)
					(name "EN")
					(number "5")
				)
				(pin unspecified line
					(at -10.16 -27.94 0)
					(length 2.54)
					(name "A0")
					(number "6")
				)
				(pin unspecified line
					(at -10.16 -19.05 0)
					(length 2.54)
					(name "PG")
					(number "7")
				)
				(pin power_in line
					(at 1.27 -33.02 90)
					(length 2.54)
					(name "PGND")
					(number "8")
				)
				(pin power_in line
					(at -10.16 -5.08 0)
					(length 2.54)
					(name "VIN")
					(number "9")
				)
				(pin unspecified line
					(at 10.16 -12.7 180)
					(length 2.54)
					(name "VOUT")
					(number "10")
				)
				(pin unspecified line
					(at 10.16 -20.32 180)
					(length 2.54)
					(name "FB")
					(number "11")
				)
				(pin unspecified line
					(at 10.16 -27.94 180)
					(length 2.54)
					(name "SS")
					(number "12")
				)
				(pin power_out line
					(at -10.16 -12.7 0)
					(length 2.54)
					(name "VCC")
					(number "13")
				)
				(pin power_in line
					(at -1.27 -33.02 90)
					(length 2.54)
					(name "AGND")
					(number "14")
				)
			)
			(embedded_fonts no)
		)
)
