(footprint "QFN-40-1EP_6x6x0.9mm_P0.5mm_EP4x4mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -4.09 -3.93 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-40-1EP_6x6x0.9mm_P0.5mm_EP4x4mm"
		(at -4.09 4.84 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -4.09 6.04 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -4.09 7.24 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -4.09 8.44 0)
		(layer "F.Fab")
	)
	(fp_text user ""
		(at 0 0 0)
		(layer "User.5")
	)
	(fp_text user ""
		(at 0 0 0)
		(layer "User.9")
	)
	(pad "" smd roundrect
		(at -1 -1)
		(size 1.6 1.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -1 1)
		(size 1.6 1.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1 -1)
		(size 1.6 1.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1 1)
		(size 1.6 1.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd oval
		(at -3.025 -2.245)
		(size 0.825 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "2" smd oval
		(at -2.94 -1.745)
		(size 1 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "3" smd oval
		(at -2.94 -1.245)
		(size 1 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "4" smd oval
		(at -2.94 -0.745)
		(size 1 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "5" smd oval
		(at -2.94 -0.245)
		(size 1 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "6" smd oval
		(at -2.94 0.255)
		(size 1 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "7" smd oval
		(at -2.94 0.755)
		(size 1 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "8" smd oval
		(at -2.94 1.255)
		(size 1 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "9" smd oval
		(at -2.94 1.755)
		(size 1 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "10" smd oval
		(at -3.025 2.255)
		(size 0.825 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "11" smd oval
		(at -2.25 3.025)
		(size 0.37 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "12" smd oval
		(at -1.75 2.94)
		(size 0.37 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "13" smd oval
		(at -1.25 2.94)
		(size 0.37 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "14" smd oval
		(at -0.75 2.94)
		(size 0.37 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "15" smd oval
		(at -0.25 2.94)
		(size 0.37 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "16" smd oval
		(at 0.25 2.94)
		(size 0.37 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "17" smd oval
		(at 0.75 2.94)
		(size 0.37 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "18" smd oval
		(at 1.25 2.94)
		(size 0.37 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "19" smd oval
		(at 1.75 2.94)
		(size 0.37 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "20" smd oval
		(at 2.25 3.025)
		(size 0.37 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "21" smd oval
		(at 3.02 2.25)
		(size 0.825 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "22" smd oval
		(at 2.94 1.755)
		(size 1 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "23" smd oval
		(at 2.94 1.255)
		(size 1 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "24" smd oval
		(at 2.94 0.755)
		(size 1 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "25" smd oval
		(at 2.94 0.255)
		(size 1 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "26" smd oval
		(at 2.94 -0.245)
		(size 1 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "27" smd oval
		(at 2.94 -0.745)
		(size 1 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "28" smd oval
		(at 2.94 -1.245)
		(size 1 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "29" smd oval
		(at 2.94 -1.745)
		(size 1 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "30" smd oval
		(at 3.03 -2.25)
		(size 0.825 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "31" smd oval
		(at 2.25 -3.015)
		(size 0.37 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "32" smd oval
		(at 1.75 -2.93)
		(size 0.37 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "33" smd oval
		(at 1.25 -2.93)
		(size 0.37 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "34" smd oval
		(at 0.75 -2.93)
		(size 0.37 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "35" smd oval
		(at 0.25 -2.93)
		(size 0.37 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "36" smd oval
		(at -0.25 -2.93)
		(size 0.37 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "37" smd oval
		(at -0.75 -2.93)
		(size 0.37 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "38" smd oval
		(at -1.25 -2.93)
		(size 0.37 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "39" smd oval
		(at -1.75 -2.93)
		(size 0.37 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "40" smd oval
		(at -2.25 -3.015)
		(size 0.37 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "41" smd rect
		(at 0 0.005)
		(size 4 4.1)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.05)
		(zone_connect 2)
	)
	(pad "42" smd rect
		(at -2.765 -2.765)
		(size 0.33 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "42" smd rect
		(at -2.765 2.765)
		(size 0.33 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "42" smd rect
		(at 2.765 -2.765)
		(size 0.33 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "42" smd rect
		(at 2.765 2.765)
		(size 0.33 0.33)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(embedded_fonts no)
	(model "antmicro_mpf5023amba0es.glb"
		(offset
			(xyz -0 -0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
