(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PF5023"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 58.42 -1.27 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PF5023"
				(at 58.42 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PF5023"
				(at 58.42 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PF5023.pdf"
				(at 58.42 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Power management integrated circuit (PMIC) for high performance applications"
				(at 58.42 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MPF5023AMBA0ES"
				(at 58.42 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "NXP"
				(at 58.42 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 58.42 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 58.42 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, VOLTAGE, REGULATOR, SWITCHING, DC-DC, CONTROLLER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PF5023_1_0"
				(pin no_connect line
					(at 40.64 -72.39 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "42")
				)
			)
			(symbol "PF5023_1_1"
				(pin input line
					(at 43.18 -22.86 180)
					(length 2.54)
					(name "SW2FB")
					(number "1")
				)
				(pin power_in line
					(at 0 -6.35 0)
					(length 2.54)
					(name "SW1IN")
					(number "2")
				)
				(pin power_out line
					(at 43.18 -15.24 180)
					(length 2.54)
					(name "SW1LX")
					(number "3")
				)
				(pin open_collector line
					(at 43.18 -25.4 180)
					(length 2.54)
					(name "SW2LX")
					(number "4")
				)
				(pin power_in line
					(at 0 -8.89 0)
					(length 2.54)
					(name "SW2IN")
					(number "5")
				)
				(pin power_out line
					(at 0 -11.43 0)
					(length 2.54)
					(name "SW3IN")
					(number "6")
				)
				(pin power_out line
					(at 43.18 -35.56 180)
					(length 2.54)
					(name "SW3LX")
					(number "7")
				)
				(pin no_connect line
					(at 40.64 -72.39 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "8")
				)
				(pin no_connect line
					(at 40.64 -72.39 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "9")
				)
				(pin no_connect line
					(at 40.64 -72.39 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "10")
				)
				(pin input line
					(at 43.18 -33.02 180)
					(length 2.54)
					(name "SW3FB")
					(number "11")
				)
				(pin no_connect line
					(at 40.64 -72.39 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "12")
				)
				(pin input line
					(at 0 -39.37 0)
					(length 2.54)
					(name "EN3")
					(number "13")
				)
				(pin no_connect line
					(at 40.64 -72.39 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "14")
				)
				(pin no_connect line
					(at 40.64 -72.39 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "15")
				)
				(pin no_connect line
					(at 40.64 -72.39 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "16")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VIN")
					(number "17")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 2.54)
					(name "AGND")
					(number "18")
				)
				(pin output line
					(at 43.18 -48.26 180)
					(length 2.54)
					(name "PGOOD1")
					(number "19")
				)
				(pin output line
					(at 43.18 -50.8 180)
					(length 2.54)
					(name "PGOOD2")
					(number "20")
				)
				(pin bidirectional line
					(at 43.18 -68.58 180)
					(length 2.54)
					(name "XFAILB")
					(number "21")
				)
				(pin input line
					(at 0 -26.67 0)
					(length 2.54)
					(name "STANDBY")
					(number "22")
				)
				(pin power_out line
					(at 43.18 -2.54 180)
					(length 2.54)
					(name "V1P5A")
					(number "23")
				)
				(pin power_out line
					(at 43.18 -5.08 180)
					(length 2.54)
					(name "V1P5D")
					(number "24")
				)
				(pin output line
					(at 43.18 -64.77 180)
					(length 2.54)
					(name "INTB")
					(number "25")
				)
				(pin output line
					(at 43.18 -45.72 180)
					(length 2.54)
					(name "PGOOD")
					(number "26")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 2.54)
					(name "SYNC")
					(number "27")
				)
				(pin passive line
					(at 0 -69.85 0)
					(length 2.54)
					(name "VDDOTP")
					(number "28")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 2.54)
					(name "SDA")
					(number "29")
				)
				(pin bidirectional line
					(at 0 -57.15 0)
					(length 2.54)
					(name "SCL")
					(number "30")
				)
				(pin input line
					(at 0 -24.13 0)
					(length 2.54)
					(name "PWRON")
					(number "31")
				)
				(pin output line
					(at 43.18 -53.34 180)
					(length 2.54)
					(name "PGOOD3")
					(number "32")
				)
				(pin no_connect line
					(at 40.64 -72.39 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "33")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 2.54)
					(name "WDI")
					(number "34")
				)
				(pin input line
					(at 0 -67.31 0)
					(length 2.54)
					(name "TBBEN")
					(number "35")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 2.54)
					(name "VDDIO")
					(number "36")
				)
				(pin output line
					(at 43.18 -60.96 180)
					(length 2.54)
					(name "RESETBMCU")
					(number "37")
				)
				(pin input line
					(at 0 -34.29 0)
					(length 2.54)
					(name "EN1")
					(number "38")
				)
				(pin input line
					(at 0 -36.83 0)
					(length 2.54)
					(name "EN2")
					(number "39")
				)
				(pin input line
					(at 43.18 -12.7 180)
					(length 2.54)
					(name "SW1FB")
					(number "40")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 2.54)
					(name "EPAD")
					(number "41")
				)
			)
			(embedded_fonts no)
		)
)
