(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MPF5302AMDA0ES"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 40.64 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MPF5302AMDA0ES"
				(at 40.64 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MPF5302AMDA0ES"
				(at 40.64 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PF5300.pdf"
				(at 40.64 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "DC-DC Switching Synchronous Step-Down Regulator, 15A, 5V in, 0.5-1.2V out"
				(at 40.64 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MPF5302AMDA0ES"
				(at 40.64 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "NXP"
				(at 40.64 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 40.64 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 40.64 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, VOLTAGE, REGULATOR, SWITCHING, DC-DC, No-RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MPF5302AMDA0ES_1_1"
				(pin power_in line
					(at 26.67 -48.26 180)
					(length 2.54)
					(name "PGND")
					(number "1")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "PVIN")
					(number "4")
				)
				(pin input line
					(at 26.67 -7.62 180)
					(length 2.54)
					(name "BOOT")
					(number "5")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 2.54)
					(name "VIN")
					(number "6")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 2.54)
					(name "STANDBY")
					(number "7")
					(alternate "SYNCIN" passive line)
				)
				(pin output line
					(at 26.67 0 180)
					(length 2.54)
					(name "PGOOD")
					(number "8")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 2.54)
					(name "PWRON")
					(number "9")
				)
				(pin power_in line
					(at 26.67 -45.72 180)
					(length 2.54)
					(name "AGND")
					(number "10")
				)
				(pin input line
					(at 26.67 -29.21 180)
					(length 2.54)
					(name "FB-")
					(number "11")
				)
				(pin input line
					(at 26.67 -26.67 180)
					(length 2.54)
					(name "FB+")
					(number "12")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 2.54)
					(name "VDDOTP")
					(number "13")
					(alternate "XFAILB" passive line)
				)
				(pin input line
					(at 0 -38.1 0)
					(length 2.54)
					(name "SCL")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "SDA")
					(number "15")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "PVIN")
					(number "16")
				)
				(pin passive line
					(at 26.67 -48.26 180)
					(length 2.54)
					(hide yes)
					(name "PGND")
					(number "17")
				)
				(pin power_out line
					(at 26.67 -11.43 180)
					(length 2.54)
					(name "LX")
					(number "21")
				)
			)
			(embedded_fonts no)
		)
)
