(footprint "QFN-20-2EP-3.5x5x1.6mm_P0.5mm_MPS_MPM3630"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(tags "MPM3630GQV-P ")
	(property "Reference" "REF**"
		(at 0.75 -4.2 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-20-2EP-3.5x5x1.6mm_P0.5mm_MPS_MPM3630"
		(at 1.65 5.2 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -2.4 7.2 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -2.4 8.4 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -2.4 9.6 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.395 -1.55)
		(size 0.8128 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.255 -0.9)
		(size 1.0922 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.255 -0.25)
		(size 1.0922 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.545 0.4)
		(size 0.508 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -1.545 1.25)
		(size 0.508 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -1 1.25)
		(size 0.583 1.954)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -1.545 2.1)
		(size 0.508 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 1.545 2.1)
		(size 0.508 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 1 1.25)
		(size 0.583 1.954)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 1.545 1.25)
		(size 0.508 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 1.545 0.4)
		(size 0.508 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 1.255 -0.25)
		(size 1.0922 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 1.255 -0.9)
		(size 1.0922 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 1.445 -1.55)
		(size 0.7112 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 1.25 -2.445 90)
		(size 0.7112 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 0.75 -2.445 90)
		(size 0.7112 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 0.25 -2.255 90)
		(size 1.0922 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -0.25 -2.255 90)
		(size 1.0922 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -0.75 -2.445 90)
		(size 0.7112 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -1.25 -2.445 90)
		(size 0.7112 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -0.25 -0.575)
		(size 0.254 0.4064)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 0.25 -0.575)
		(size 0.254 0.4064)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(zone
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 0.575 -0.97) (xy -0.575 -0.97) (xy -0.575 -0.18) (xy 0.575 -0.18)
			)
		)
	)
	(embedded_fonts no)
	(model "antmicro_mpm3630gqv_p.glb"
		(offset
			(xyz -1.5 -2.5 0.11)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
