(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MPM3630GQV-P"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 34.29 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MPM3630GQV-P"
				(at 34.29 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MPM3630GQV-P"
				(at 34.29 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.monolithicpower.com/en/documentview/productdocument/index/version/2/document_type/Datasheet/lang/en/sku/MPM3630GQV/document_id/2114/"
				(at 34.29 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "DC-DC Switching Synchronous Step-Down Regulator,  4.5V-18V in, 0.6V-16.2V/3A out, QFN-20"
				(at 34.29 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 34.29 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 34.29 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MPM3630GQV-P"
				(at 34.29 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Monolithic Power Systems"
				(at 34.29 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, VOLTAGE, REGULATOR, SWITCHING, DC-DC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MPM3630GQV-P_1_1"
				(pin input line
					(at 21.59 -12.7 180)
					(length 2.54)
					(name "FB")
					(number "1")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 2.54)
					(name "VCC")
					(number "2")
				)
				(pin power_out line
					(at 21.59 -20.32 180)
					(length 2.54)
					(name "AGND")
					(number "3")
				)
				(pin output line
					(at 21.59 -2.54 180)
					(length 2.54)
					(name "SW")
					(number "4")
				)
				(pin passive line
					(at 21.59 -2.54 180)
					(length 2.54)
					(name "SW")
					(number "5")
				)
				(pin passive line
					(at 21.59 -2.54 180)
					(length 2.54)
					(name "SW")
					(number "6")
				)
				(pin output line
					(at 21.59 -5.08 180)
					(length 2.54)
					(name "OUT")
					(number "7")
				)
				(pin passive line
					(at 21.59 -5.08 180)
					(length 2.54)
					(name "OUT")
					(number "8")
				)
				(pin passive line
					(at 21.59 -5.08 180)
					(length 2.54)
					(name "OUT")
					(number "9")
				)
				(pin no_connect line
					(at 19.05 -17.78 180)
					(length 2.54)
					(name "NC")
					(number "10")
				)
				(pin unspecified line
					(at 21.59 0 180)
					(length 2.54)
					(name "BST")
					(number "11")
				)
				(pin power_out line
					(at 21.59 -22.86 180)
					(length 2.54)
					(name "PGND")
					(number "12")
				)
				(pin passive line
					(at 21.59 -22.86 180)
					(length 2.54)
					(name "PGND")
					(number "13")
				)
				(pin passive line
					(at 21.59 -22.86 180)
					(length 2.54)
					(name "PGND")
					(number "14")
				)
				(pin no_connect line
					(at 19.05 -15.24 180)
					(length 2.54)
					(name "NC")
					(number "15")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "IN")
					(number "16")
				)
				(pin unspecified line
					(at 0 -10.16 0)
					(length 2.54)
					(name "EN/SYNC")
					(number "17")
				)
				(pin unspecified line
					(at 0 -12.7 0)
					(length 2.54)
					(name "PG")
					(number "18")
				)
				(pin no_connect line
					(at 19.05 -10.16 180)
					(length 2.54)
					(name "NC")
					(number "19")
				)
				(pin no_connect line
					(at 19.05 -7.62 180)
					(length 2.54)
					(name "NC")
					(number "20")
				)
			)
			(embedded_fonts no)
		)
)
