(footprint "LGA-33_7x7mm_P0.65mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -4.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "LGA-33_7x7mm_P0.65mm"
		(at 0 5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_paste_margin_ratio -0.1)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -4.35 7.299 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -4.35 8.499 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -4.35 9.699 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -3.138 -1.625 90)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -3.138 -0.975 90)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -3.138 -0.328 90)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -3.138 0.325 90)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -3.138 0.972 90)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -3.138 1.624 90)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -2.926 3.136 180)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -2.275 3.136 180)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -1.625 3.136)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -0.975 3.136)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -0.328 3.136)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 0.325 3.136)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 0.972 3.136)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 1.624 3.136)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 2.273 3.136)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 2.922 3.136)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 3.136 1.624 90)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 3.136 0.972 90)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 3.136 0.325 90)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 3.136 -0.328 90)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 3.136 -0.975 90)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 3.136 -1.625 90)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 2.922 -3.138 180)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 2.273 -3.138 180)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 1.624 -3.138)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 0.972 -3.138)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 0.325 -3.138)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at -0.328 -3.138)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at -0.975 -3.138)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at -1.625 -3.138)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at -2.275 -3.138)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at -2.926 -3.138)
		(size 0.3 1.125)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at -0.863 -0.863)
		(size 1.725 1.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.1)
	)
	(pad "33" smd rect
		(at -0.863 0.86)
		(size 1.725 1.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.1)
	)
	(pad "33" smd rect
		(at 0.86 -0.863)
		(size 1.725 1.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.1)
	)
	(pad "33" smd rect
		(at 0.86 0.86)
		(size 1.725 1.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.1)
	)
	(embedded_fonts no)
	(model "antmicro_mpm54304gmn_0000.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
