(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MPM54304GMN-0004"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 46.99 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MPM54304GMN-0004"
				(at 46.99 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MPM54304GMN-0004"
				(at 46.99 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.monolithicpower.com/en/documentview/productdocument/index/version/2/document_type/Datasheet/lang/en/sku/MPM54304/document_id/4982/"
				(at 46.99 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "DC-DC Switching Synchronous Step-Down Regulator, Multi Output, 4-16V in, 1V/3.3V, 4.2/3A out, LGA33"
				(at 46.99 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MPM54304GMN-0004"
				(at 46.99 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Monolithic Power Systems"
				(at 46.99 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 46.99 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 46.99 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, VOLTAGE, REGULATOR, SWITCHING, DC-DC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "CP_48_13_ADI CP_48_13_ADI-M CP_48_13_ADI-L"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MPM54304GMN-0004_1_1"
				(pin power_out line
					(at 27.94 -22.86 180)
					(length 2.54)
					(name "VOUT3")
					(number "1")
				)
				(pin power_in line
					(at 0 -35.56 0)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 2.54)
					(name "SDA")
					(number "3")
				)
				(pin input line
					(at 0 -21.59 0)
					(length 2.54)
					(name "SCL")
					(number "4")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "5")
				)
				(pin input line
					(at 27.94 -17.78 180)
					(length 2.54)
					(name "FB2")
					(number "6")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "7")
				)
				(pin power_out line
					(at 27.94 -12.7 180)
					(length 2.54)
					(name "VOUT2")
					(number "8")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 2.54)
					(hide yes)
					(name "VOUT2")
					(number "9")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "10")
				)
				(pin power_out line
					(at 27.94 -15.24 180)
					(length 2.54)
					(name "SW2")
					(number "11")
				)
				(pin power_out line
					(at 27.94 -2.54 180)
					(length 2.54)
					(name "SW1")
					(number "12")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "13")
				)
				(pin power_out line
					(at 27.94 0 180)
					(length 2.54)
					(name "VOUT1")
					(number "14")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 2.54)
					(hide yes)
					(name "VOUT1")
					(number "15")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "16")
				)
				(pin power_out line
					(at 27.94 -7.62 180)
					(length 2.54)
					(name "SGND1")
					(number "17")
				)
				(pin input line
					(at 27.94 -5.08 180)
					(length 2.54)
					(name "FB1")
					(number "18")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "EN/SYNCI")
					(number "19")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "20")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "21")
				)
				(pin power_out line
					(at 27.94 -33.02 180)
					(length 2.54)
					(name "VOUT4")
					(number "22")
				)
				(pin passive line
					(at 27.94 -33.02 180)
					(length 2.54)
					(hide yes)
					(name "VOUT4")
					(number "23")
				)
				(pin input line
					(at 27.94 -35.56 180)
					(length 2.54)
					(name "FB4")
					(number "24")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VCC")
					(number "25")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "GPIO")
					(number "26")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "27")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VIN")
					(number "28")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VIN")
					(number "29")
				)
				(pin power_out line
					(at 27.94 -27.94 180)
					(length 2.54)
					(name "SGND2")
					(number "30")
				)
				(pin input line
					(at 27.94 -25.4 180)
					(length 2.54)
					(name "FB3")
					(number "31")
				)
				(pin passive line
					(at 27.94 -22.86 180)
					(length 2.54)
					(hide yes)
					(name "VOUT3")
					(number "32")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "33")
				)
			)
			(embedded_fonts no)
		)
)
