(footprint "MS621FE-FL11E"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -5.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "MS621FE-FL11E"
		(at -0.001 6.2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -3.501 8.2 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -3.501 9.4 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -3.501 11.8 0)
		(layer "F.Fab")
	)
	(fp_text user "COPPER KEEPOUT"
		(at -0.2 -3.14 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -0.75 -4.05 270)
		(size 1.8 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 0.75 -4.05 270)
		(size 1.8 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(zone
		(layers "F.Cu" "F.CrtYd")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(keepout
			(tracks allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy -1.16 2.5) (xy -1.16 -3.14) (xy 1.16 -3.14) (xy 1.16 2.5)
			)
		)
	)
	(embedded_fonts no)
	(model "antmicro_ms621fe_fl11e.glb"
		(offset
			(xyz -1 -8.75 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 -90)
		)
	)
)
