(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "NCP451AFCT2G"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 30.48 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "NCP451AFCT2G"
				(at 30.48 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "NCP451AFCT2G"
				(at 30.48 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/308/NCP451_D-1812749.pdf"
				(at 30.48 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Power Load Switch, High Side, Active High, 1 Output, 0.012 ohm On State, 5.5 V supp, 3 A, WLCSP-6"
				(at 30.48 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "NCP451AFCT2G"
				(at 30.48 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "ON Semiconductor"
				(at 30.48 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 30.48 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 30.48 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "NCP451AFCT2G_1_1"
				(pin power_out line
					(at 15.24 0 180)
					(length 2.54)
					(name "OUT")
					(number "A1")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "IN")
					(number "A2")
				)
				(pin passive line
					(at 15.24 0 180)
					(length 2.54)
					(hide yes)
					(name "OUT")
					(number "B1")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "IN")
					(number "B2")
				)
				(pin power_in line
					(at 15.24 -5.08 180)
					(length 2.54)
					(name "GND")
					(number "C1")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "EN")
					(number "C2")
				)
			)
			(embedded_fonts no)
		)
)
