(footprint "WLCSP-45_2.175x3.635mm_Layout5x9_P0.39x0.42mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -0.725 -0.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "WLCSP-45_2.175x3.635mm_Layout5x9_P0.39x0.42mm"
		(at -1.125 5.075 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -1.075 6.137 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -1.075 7.337 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -1.075 8.537 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at 0 0)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd circle
		(at 0.42 0)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd circle
		(at 0.84 0)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd circle
		(at 1.26 0)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd circle
		(at 1.68 0)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd circle
		(at 0 0.39)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd circle
		(at 0.42 0.39)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd circle
		(at 0.84 0.39)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd circle
		(at 1.26 0.39)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B5" smd circle
		(at 1.68 0.39)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd circle
		(at 0 0.78)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd circle
		(at 0.42 0.78)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C3" smd circle
		(at 0.84 0.78)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C4" smd circle
		(at 1.26 0.78)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C5" smd circle
		(at 1.68 0.78)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D1" smd circle
		(at 0 1.17)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D2" smd circle
		(at 0.42 1.17)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D3" smd circle
		(at 0.84 1.17)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D4" smd circle
		(at 1.26 1.17)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D5" smd circle
		(at 1.68 1.17)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E1" smd circle
		(at 0 1.56)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E2" smd circle
		(at 0.42 1.56)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E3" smd circle
		(at 0.84 1.56)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E4" smd circle
		(at 1.26 1.56)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E5" smd circle
		(at 1.68 1.56)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F1" smd circle
		(at 0 1.95)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F2" smd circle
		(at 0.42 1.95)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F3" smd circle
		(at 0.84 1.95)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F4" smd circle
		(at 1.26 1.95)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F5" smd circle
		(at 1.68 1.95)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G1" smd circle
		(at 0 2.34)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G2" smd circle
		(at 0.42 2.34)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G3" smd circle
		(at 0.84 2.34)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G4" smd circle
		(at 1.26 2.34)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G5" smd circle
		(at 1.68 2.34)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H1" smd circle
		(at 0 2.73)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H2" smd circle
		(at 0.42 2.73)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H3" smd circle
		(at 0.84 2.73)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H4" smd circle
		(at 1.26 2.73)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H5" smd circle
		(at 1.68 2.73)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J1" smd circle
		(at 0 3.12)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J2" smd circle
		(at 0.42 3.12)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J3" smd circle
		(at 0.84 3.12)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J4" smd circle
		(at 1.26 3.12)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J5" smd circle
		(at 1.68 3.12)
		(size 0.21 0.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_npm6001_caaa_r7.glb"
		(offset
			(xyz -4.85 -2.475 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 90)
		)
	)
)
