(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "nPM6001"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 48.26 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "nPM6001"
				(at 48.26 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "nPM6001"
				(at 48.26 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/297/nPM6001_PS_v1_0-3159402.pdf"
				(at 48.26 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Compact DC-DC Switching Synchronous Step-Down Regulator, Multi Output, 5.5-3.0V in"
				(at 48.26 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "nPM6001-CAAA-R7"
				(at 48.26 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Nordic Semiconductor"
				(at 48.26 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 48.26 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 48.26 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, VOLTAGE, REGULATOR, SWITCHING, DC-DC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "nPM6001_1_1"
				(pin power_in line
					(at 0 -12.7 0)
					(length 2.54)
					(name "VIN_BUCK2")
					(number "A1")
				)
				(pin passive line
					(at 33.02 -22.86 180)
					(length 2.54)
					(name "SW2")
					(number "A2")
				)
				(pin power_in line
					(at 33.02 -76.2 180)
					(length 2.54)
					(name "AVSS1_2")
					(number "A3")
				)
				(pin passive line
					(at 33.02 -12.7 180)
					(length 2.54)
					(name "SW1")
					(number "A4")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "VIN_BUCK1")
					(number "A5")
				)
				(pin passive line
					(at 33.02 -25.4 180)
					(length 2.54)
					(name "VO2")
					(number "B1")
				)
				(pin passive line
					(at 0 -34.29 0)
					(length 2.54)
					(name "ENABLE")
					(number "B2")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 2.54)
					(name "RESERVED")
					(number "B3")
				)
				(pin no_connect line
					(at 2.54 -76.2 0)
					(length 2.54)
					(name "NC")
					(number "B4")
				)
				(pin passive line
					(at 33.02 -15.24 180)
					(length 2.54)
					(name "VO1")
					(number "B5")
				)
				(pin power_in line
					(at 33.02 -53.34 180)
					(length 2.54)
					(name "VIN_LDO0")
					(number "C1")
				)
				(pin bidirectional line
					(at 0 -67.31 0)
					(length 2.54)
					(name "GPIO0")
					(number "C2")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 2.54)
					(name "RESERVED")
					(number "C3")
				)
				(pin passive line
					(at 0 -39.37 0)
					(length 2.54)
					(name "VDD_TWI")
					(number "C4")
				)
				(pin passive line
					(at 33.02 -45.72 180)
					(length 2.54)
					(name "VLDO1")
					(number "C5")
				)
				(pin passive line
					(at 33.02 -55.88 180)
					(length 2.54)
					(name "VLDO0")
					(number "D1")
				)
				(pin bidirectional line
					(at 0 -72.39 0)
					(length 2.54)
					(name "GPIO2")
					(number "D2")
				)
				(pin bidirectional line
					(at 0 -69.85 0)
					(length 2.54)
					(name "GPIO1")
					(number "D3")
				)
				(pin input line
					(at 0 -29.21 0)
					(length 2.54)
					(name "~{INT}")
					(number "D4")
				)
				(pin power_in line
					(at 33.02 -43.18 180)
					(length 2.54)
					(name "VIN_LDO1")
					(number "D5")
				)
				(pin power_in line
					(at 0 -24.13 0)
					(length 2.54)
					(name "VIN_GPIO")
					(number "E1")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 2.54)
					(name "SDA")
					(number "E2")
				)
				(pin input line
					(at 0 -49.53 0)
					(length 2.54)
					(name "SCL")
					(number "E3")
				)
				(pin no_connect line
					(at 2.54 -78.74 0)
					(length 2.54)
					(name "NC")
					(number "E4")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 2.54)
					(name "RESERVED")
					(number "E5")
				)
				(pin power_in line
					(at 33.02 -81.28 180)
					(length 2.54)
					(name "AVSS")
					(number "F1")
				)
				(pin power_in line
					(at 33.02 -83.82 180)
					(length 2.54)
					(name "AVSS_ANA")
					(number "F2")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VIN_ANA")
					(number "F3")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 2.54)
					(name "RESERVED")
					(number "F4")
				)
				(pin passive line
					(at 0 -57.15 0)
					(length 2.54)
					(name "BUCK_MODE1")
					(number "F5")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VIN")
					(number "G1")
				)
				(pin passive line
					(at 0 -54.61 0)
					(length 2.54)
					(name "BUCK_MODE0")
					(number "G2")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 2.54)
					(name "RESERVED")
					(number "G3")
				)
				(pin passive line
					(at 0 -59.69 0)
					(length 2.54)
					(name "BUCK_MODE2")
					(number "G4")
				)
				(pin passive line
					(at 33.02 -5.08 180)
					(length 2.54)
					(name "VO0_IN")
					(number "G5")
				)
				(pin passive line
					(at 33.02 -35.56 180)
					(length 2.54)
					(name "VO3")
					(number "H1")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 2.54)
					(name "RESERVED")
					(number "H2")
				)
				(pin power_in line
					(at 33.02 -73.66 180)
					(length 2.54)
					(name "AVSS0")
					(number "H3")
				)
				(pin input line
					(at 0 -31.75 0)
					(length 2.54)
					(name "READY")
					(number "H4")
				)
				(pin passive line
					(at 33.02 -2.54 180)
					(length 2.54)
					(name "VO0")
					(number "H5")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "VIN_BUCK3")
					(number "J1")
				)
				(pin passive line
					(at 33.02 -33.02 180)
					(length 2.54)
					(name "SW3")
					(number "J2")
				)
				(pin power_in line
					(at 33.02 -78.74 180)
					(length 2.54)
					(name "AVSS3")
					(number "J3")
				)
				(pin passive line
					(at 33.02 0 180)
					(length 2.54)
					(name "SW0")
					(number "J4")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VIN_BUCK0")
					(number "J5")
				)
			)
			(embedded_fonts no)
		)
)
