(footprint "antmicro_pca9543apw"
  (version 20240108) (generator "partreel")
  (layer "F.Cu")
  (descr "TSSOP-14_4.4x5mm_P0.65mm replacement land pattern per manufacturer datasheet: TI SLCS006Z land pattern drawing 4220202/B (12/2023), PDF p.52; dimensions re-measured from the drawing's 10X vector geometry (row span 5.800 c-c confirmed)")
  (attr smd)
  (fp_text reference "REF**" (at 0 -3.95) (layer "F.SilkS"))
  (fp_text value "VAL**" (at 0 3.95) (layer "F.Fab"))
  (pad "1" smd rect (at -2.9 -1.95) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at -2.9 -1.3) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at -2.9 -0.65) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at -2.9 0) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd rect (at -2.9 0.65) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "6" smd rect (at -2.9 1.3) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "7" smd rect (at -2.9 1.95) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "8" smd rect (at 2.9 1.95) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "9" smd rect (at 2.9 1.3) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "10" smd rect (at 2.9 0.65) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "11" smd rect (at 2.9 0) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "12" smd rect (at 2.9 -0.65) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "13" smd rect (at 2.9 -1.3) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "14" smd rect (at 2.9 -1.95) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask"))
)
