(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PI3C3125_TSSOP"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 39.37 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PI3C3125_TSSOP"
				(at 39.37 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PI3C3125_TSSOP"
				(at 39.37 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PI3C3125-3126.pdf"
				(at 39.37 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "2.5V/3.3V, High Bandwidth, Hot Insertion,4-Bit, 2-Port Bus Switch with Individual Enables"
				(at 39.37 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "PI3C3125LEX"
				(at 39.37 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Diodes Incorporated"
				(at 39.37 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 39.37 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 39.37 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, LOGIC, IC, MUX"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PI3C3125_TSSOP_1_1"
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "~{BE}_{0}")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 2.54)
					(name "A_{0}")
					(number "2")
				)
				(pin bidirectional line
					(at 15.24 -3.81 180)
					(length 2.54)
					(name "B_{0}")
					(number "3")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "~{BE}_{1}")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "A_{1}")
					(number "5")
				)
				(pin bidirectional line
					(at 15.24 -10.16 180)
					(length 2.54)
					(name "B_{1}")
					(number "6")
				)
				(pin power_in line
					(at 0 -29.21 0)
					(length 2.54)
					(name "GND")
					(number "7")
				)
				(pin bidirectional line
					(at 15.24 -16.51 180)
					(length 2.54)
					(name "B_{2}")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 2.54)
					(name "A_{2}")
					(number "9")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 2.54)
					(name "~{BE}_{2}")
					(number "10")
				)
				(pin bidirectional line
					(at 15.24 -22.86 180)
					(length 2.54)
					(name "B_{3}")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "A_{3}")
					(number "12")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "~{BE}_{3}")
					(number "13")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{CC}")
					(number "14")
				)
			)
			(embedded_fonts no)
		)
)
